   UDP-MIB DEFINITIONS ::= BEGIN

   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, Integer32, Counter32, Counter64,
       Unsigned32, IpAddress, mib-2       FROM SNMPv2-SMI
       MODULE-COMPLIANCE, OBJECT-GROUP    FROM SNMPv2-CONF
       InetAddress, InetAddressType,
       InetPortNumber                     FROM INET-ADDRESS-MIB;

   udpMIB MODULE-IDENTITY
       LAST-UPDATED "200505200000Z"  -- May 20, 2005
       ORGANIZATION
              "IETF IPv6 Working Group
               http://www.ietf.org/html.charters/ipv6-charter.html"
       CONTACT-INFO
              "Bill Fenner (editor)

               AT&T Labs -- Research
               75 Willow Rd.
               Menlo Park, CA 94025

               Phone: +1 650 330-7893
               Email: <fenner@research.att.com>

               John Flick (editor)

               Hewlett-Packard Company
               8000 Foothills Blvd. M/S 5557
               Roseville, CA 95747

               Phone: +1 916 785 4018
               Email: <john.flick@hp.com>

               Send comments to <ipv6@ietf.org>"

       DESCRIPTION
              "The MIB module for managing UDP implementations.
               Copyright (C) The Internet Society (2005).  This
               version of this MIB module is part of RFC 4113;
               see the RFC itself for full legal notices."
       REVISION      "200505200000Z"  -- May 20, 2005
       DESCRIPTION
              "IP version neutral revision, incorporating the
               following revisions:

               - Added udpHCInDatagrams and udpHCOutDatagrams in order
                 to provide high-capacity counters for fast networks.
               - Added text to the descriptions of all counter objects
                 to indicate how discontinuities are detected.
               - Deprecated the IPv4-specific udpTable and replaced it
                 with the version neutral udpEndpointTable.  This
                 table includes support for connected UDP endpoints
                 and support for identification of the operating
                 system process associated with a UDP endpoint.
               - Deprecated the udpGroup and replaced it with object
                 groups representing the current set of objects.
               - Deprecated udpMIBCompliance and replaced it with
                 udpMIBCompliance2, which includes the compliance
                 information for the new object groups.

               This version published as RFC 4113."
       REVISION      "199411010000Z"    -- November 1, 1994
       DESCRIPTION
              "Initial SMIv2 version, published as RFC 2013."
       REVISION      "199103310000Z"    -- March 31, 1991
       DESCRIPTION
              "The initial revision of this MIB module was part of
               MIB-II, published as RFC 1213."
       ::= { mib-2 50 }

   -- the UDP group

   udp      OBJECT IDENTIFIER ::= { mib-2 7 }

   udpInDatagrams OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
              "The total number of UDP datagrams delivered to UDP
               users.

               Discontinuities in the value of this counter can occur
               at re-initialization of the management system, and at
               other times as indicated by discontinuities in the
               value of sysUpTime."
       ::= { udp 1 }

   udpNoPorts OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
              "The total number of received UDP datagrams for which
               there was no application at the destination port.

               Discontinuities in the value of this counter can occur
               at re-initialization of the management system, and at
               other times as indicated by discontinuities in the
               value of sysUpTime."
       ::= { udp 2 }

   udpInErrors OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
              "The number of received UDP datagrams that could not be
               delivered for reasons other than the lack of an
               application at the destination port.

               Discontinuities in the value of this counter can occur
               at re-initialization of the management system, and at
               other times as indicated by discontinuities in the
               value of sysUpTime."
       ::= { udp 3 }

   udpOutDatagrams OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
              "The total number of UDP datagrams sent from this
               entity.

               Discontinuities in the value of this counter can occur
               at re-initialization of the management system, and at
               other times as indicated by discontinuities in the
               value of sysUpTime."
       ::= { udp 4 }

   udpHCInDatagrams OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
              "The total number of UDP datagrams delivered to UDP
               users, for devices that can receive more than 1
               million UDP datagrams per second.

               Discontinuities in the value of this counter can occur
               at re-initialization of the management system, and at
               other times as indicated by discontinuities in the
               value of sysUpTime."
       ::= { udp 8 }

   udpHCOutDatagrams OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
              "The total number of UDP datagrams sent from this
               entity, for devices that can transmit more than 1
               million UDP datagrams per second.

               Discontinuities in the value of this counter can occur
               at re-initialization of the management system, and at
               other times as indicated by discontinuities in the
               value of sysUpTime."
       ::= { udp 9 }

   --
   -- { udp 6 } was defined as the ipv6UdpTable in RFC2454's
   -- IPV6-UDP-MIB.  This RFC obsoletes RFC 2454, so { udp 6 } is
   -- obsoleted.
   --

   -- The UDP "Endpoint" table.

   udpEndpointTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF UdpEndpointEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
              "A table containing information about this entity's UDP
               endpoints on which a local application is currently
               accepting or sending datagrams.

               The address type in this table represents the address
               type used for the communication, irrespective of the
               higher-layer abstraction.  For example, an application
               using IPv6 'sockets' to communicate via IPv4 between
               ::ffff:10.0.0.1 and ::ffff:10.0.0.2 would use
               InetAddressType ipv4(1).

               Unlike the udpTable in RFC 2013, this table also allows
               the representation of an application that completely
               specifies both local and remote addresses and ports.  A
               listening application is represented in three possible
               ways:

               1) An application that is willing to accept both IPv4
                  and IPv6 datagrams is represented by a
                  udpEndpointLocalAddressType of unknown(0) and a
                  udpEndpointLocalAddress of ''h (a zero-length
                  octet-string).

               2) An application that is willing to accept only IPv4
                  or only IPv6 datagrams is represented by a
                  udpEndpointLocalAddressType of the appropriate
                  address type and a udpEndpointLocalAddress of
                  '0.0.0.0' or '::' respectively.

               3) An application that is listening for datagrams only
                  for a specific IP address but from any remote
                  system is represented by a
                  udpEndpointLocalAddressType of the appropriate
                  address type, with udpEndpointLocalAddress
                  specifying the local address.

               In all cases where the remote is a wildcard, the
               udpEndpointRemoteAddressType is unknown(0), the
               udpEndpointRemoteAddress is ''h (a zero-length
               octet-string), and the udpEndpointRemotePort is 0.

               If the operating system is demultiplexing UDP packets
               by remote address and port, or if the application has
               'connected' the socket specifying a default remote
               address and port, the udpEndpointRemote* values should
               be used to reflect this."
       ::= { udp 7 }

   udpEndpointEntry OBJECT-TYPE
       SYNTAX     UdpEndpointEntry
       MAX-ACCESS not-accessible
       STATUS     current

       DESCRIPTION
              "Information about a particular current UDP endpoint.

               Implementers need to be aware that if the total number
               of elements (octets or sub-identifiers) in
               udpEndpointLocalAddress and udpEndpointRemoteAddress
               exceeds 111, then OIDs of column instances in this table
               will have more than 128 sub-identifiers and cannot be
               accessed using SNMPv1, SNMPv2c, or SNMPv3."
       INDEX   { udpEndpointLocalAddressType,
                 udpEndpointLocalAddress,
                 udpEndpointLocalPort,
                 udpEndpointRemoteAddressType,
                 udpEndpointRemoteAddress,
                 udpEndpointRemotePort,
                 udpEndpointInstance }
       ::= { udpEndpointTable 1 }

   UdpEndpointEntry ::= SEQUENCE {
           udpEndpointLocalAddressType   InetAddressType,
           udpEndpointLocalAddress       InetAddress,
           udpEndpointLocalPort          InetPortNumber,
           udpEndpointRemoteAddressType  InetAddressType,
           udpEndpointRemoteAddress      InetAddress,
           udpEndpointRemotePort         InetPortNumber,
           udpEndpointInstance           Unsigned32,
           udpEndpointProcess            Unsigned32
       }

   udpEndpointLocalAddressType OBJECT-TYPE
       SYNTAX     InetAddressType
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
              "The address type of udpEndpointLocalAddress.  Only
               IPv4, IPv4z, IPv6, and IPv6z addresses are expected, or
               unknown(0) if datagrams for all local IP addresses are
               accepted."
       ::= { udpEndpointEntry 1 }

   udpEndpointLocalAddress OBJECT-TYPE
       SYNTAX     InetAddress
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
              "The local IP address for this UDP endpoint.

               The value of this object can be represented in three

               possible ways, depending on the characteristics of the
               listening application:

               1. For an application that is willing to accept both
                  IPv4 and IPv6 datagrams, the value of this object
                  must be ''h (a zero-length octet-string), with
                  the value of the corresponding instance of the
                  udpEndpointLocalAddressType object being unknown(0).

               2. For an application that is willing to accept only IPv4
                  or only IPv6 datagrams, the value of this object
                  must be '0.0.0.0' or '::', respectively, while the
                  corresponding instance of the
                  udpEndpointLocalAddressType object represents the
                  appropriate address type.

               3. For an application that is listening for data
                  destined only to a specific IP address, the value
                  of this object is the specific IP address for which
                  this node is receiving packets, with the
                  corresponding instance of the
                  udpEndpointLocalAddressType object representing the
                  appropriate address type.

               As this object is used in the index for the
               udpEndpointTable, implementors of this table should be
               careful not to create entries that would result in OIDs
               with more than 128 subidentifiers; else the information
               cannot be accessed using SNMPv1, SNMPv2c, or SNMPv3."
       ::= { udpEndpointEntry 2 }

   udpEndpointLocalPort OBJECT-TYPE
       SYNTAX     InetPortNumber
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
              "The local port number for this UDP endpoint."
       ::= { udpEndpointEntry 3 }

   udpEndpointRemoteAddressType OBJECT-TYPE
       SYNTAX     InetAddressType
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
              "The address type of udpEndpointRemoteAddress.  Only
               IPv4, IPv4z, IPv6, and IPv6z addresses are expected, or
               unknown(0) if datagrams for all remote IP addresses are
               accepted.  Also, note that some combinations of

               udpEndpointLocalAdressType and
               udpEndpointRemoteAddressType are not supported.  In
               particular, if the value of this object is not
               unknown(0), it is expected to always refer to the
               same IP version as udpEndpointLocalAddressType."
       ::= { udpEndpointEntry 4 }

   udpEndpointRemoteAddress OBJECT-TYPE
       SYNTAX     InetAddress
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
              "The remote IP address for this UDP endpoint.  If
               datagrams from any remote system are to be accepted,
               this value is ''h (a zero-length octet-string).
               Otherwise, it has the type described by
               udpEndpointRemoteAddressType and is the address of the
               remote system from which datagrams are to be accepted
               (or to which all datagrams will be sent).

               As this object is used in the index for the
               udpEndpointTable, implementors of this table should be
               careful not to create entries that would result in OIDs
               with more than 128 subidentifiers; else the information
               cannot be accessed using SNMPv1, SNMPv2c, or SNMPv3."
       ::= { udpEndpointEntry 5 }

   udpEndpointRemotePort OBJECT-TYPE
       SYNTAX     InetPortNumber
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
              "The remote port number for this UDP endpoint.  If
               datagrams from any remote system are to be accepted,
               this value is zero."
       ::= { udpEndpointEntry 6 }

   udpEndpointInstance OBJECT-TYPE
       SYNTAX     Unsigned32 (1..'ffffffff'h)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
              "The instance of this tuple.  This object is used to
               distinguish among multiple processes 'connected' to
               the same UDP endpoint.  For example, on a system
               implementing the BSD sockets interface, this would be
               used to support the SO_REUSEADDR and SO_REUSEPORT
               socket options."

       ::= { udpEndpointEntry 7 }

   udpEndpointProcess OBJECT-TYPE
       SYNTAX     Unsigned32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
              "The system's process ID for the process associated with
               this endpoint, or zero if there is no such process.
               This value is expected to be the same as
               HOST-RESOURCES-MIB::hrSWRunIndex or SYSAPPL-MIB::
               sysApplElmtRunIndex for some row in the appropriate
               tables."
       ::= { udpEndpointEntry 8 }

   -- The deprecated UDP Listener table

   -- The deprecated UDP listener table only contains information
   -- about this entity's IPv4 UDP end-points on which a local
   -- application is currently accepting datagrams.  It does not
   -- provide more detailed connection information, or information
   -- about IPv6 endpoints.

   udpTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF UdpEntry
       MAX-ACCESS not-accessible
       STATUS     deprecated
       DESCRIPTION
              "A table containing IPv4-specific UDP listener
               information.  It contains information about all local
               IPv4 UDP end-points on which an application is
               currently accepting datagrams.  This table has been
               deprecated in favor of the version neutral
               udpEndpointTable."
       ::= { udp 5 }

   udpEntry OBJECT-TYPE
       SYNTAX     UdpEntry
       MAX-ACCESS not-accessible
       STATUS     deprecated
       DESCRIPTION
              "Information about a particular current UDP listener."
       INDEX   { udpLocalAddress, udpLocalPort }
       ::= { udpTable 1 }

   UdpEntry ::= SEQUENCE {
       udpLocalAddress   IpAddress,
       udpLocalPort      Integer32

   }

   udpLocalAddress OBJECT-TYPE
       SYNTAX     IpAddress
       MAX-ACCESS read-only
       STATUS     deprecated
       DESCRIPTION
              "The local IP address for this UDP listener.  In the
               case of a UDP listener that is willing to accept
               datagrams for any IP interface associated with the
               node, the value 0.0.0.0 is used."
       ::= { udpEntry 1 }

   udpLocalPort OBJECT-TYPE
       SYNTAX     Integer32 (0..65535)
       MAX-ACCESS read-only
       STATUS     deprecated
       DESCRIPTION
              "The local port number for this UDP listener."
       ::= { udpEntry 2 }

   -- conformance information

   udpMIBConformance OBJECT IDENTIFIER ::= { udpMIB 2 }
   udpMIBCompliances OBJECT IDENTIFIER ::= { udpMIBConformance 1 }
   udpMIBGroups      OBJECT IDENTIFIER ::= { udpMIBConformance 2 }

   -- compliance statements

   udpMIBCompliance2 MODULE-COMPLIANCE
       STATUS     current
       DESCRIPTION
              "The compliance statement for systems that implement
               UDP.

               There are a number of INDEX objects that cannot be
               represented in the form of OBJECT clauses in SMIv2, but
               for which we have the following compliance
               requirements, expressed in OBJECT clause form in this
               description clause:

               -- OBJECT      udpEndpointLocalAddressType
               -- SYNTAX      InetAddressType { unknown(0), ipv4(1),
               --                               ipv6(2), ipv4z(3),
               --                               ipv6z(4) }
               -- DESCRIPTION
               --     Support for dns(5) is not required.
               -- OBJECT      udpEndpointLocalAddress

               -- SYNTAX      InetAddress (SIZE(0|4|8|16|20))
               -- DESCRIPTION
               --     Support is only required for zero-length
               --     octet-strings, and for scoped and unscoped
               --     IPv4 and IPv6 addresses.
               -- OBJECT      udpEndpointRemoteAddressType
               -- SYNTAX      InetAddressType { unknown(0), ipv4(1),
               --                               ipv6(2), ipv4z(3),
               --                               ipv6z(4) }
               -- DESCRIPTION
               --     Support for dns(5) is not required.
               -- OBJECT      udpEndpointRemoteAddress
               -- SYNTAX      InetAddress (SIZE(0|4|8|16|20))
               -- DESCRIPTION
               --     Support is only required for zero-length
               --     octet-strings, and for scoped and unscoped
               --     IPv4 and IPv6 addresses.
              "
       MODULE  -- this module
            MANDATORY-GROUPS { udpBaseGroup, udpEndpointGroup }
            GROUP       udpHCGroup
            DESCRIPTION
                   "This group is mandatory for systems that
                    are capable of receiving or transmitting more than
                    1 million UDP datagrams per second.  1 million
                    datagrams per second will cause a Counter32 to
                    wrap in just over an hour."
       ::= { udpMIBCompliances 2 }

   udpMIBCompliance MODULE-COMPLIANCE
       STATUS     deprecated
       DESCRIPTION
              "The compliance statement for IPv4-only systems that
               implement UDP.  For IP version independence, this
               compliance statement is deprecated in favor of
               udpMIBCompliance2.  However, agents are still
               encouraged to implement these objects in order to
               interoperate with the deployed base of managers."
       MODULE  -- this module
           MANDATORY-GROUPS { udpGroup }
       ::= { udpMIBCompliances 1 }

   -- units of conformance

   udpGroup OBJECT-GROUP
       OBJECTS   { udpInDatagrams, udpNoPorts,
                   udpInErrors, udpOutDatagrams,
                   udpLocalAddress, udpLocalPort }

       STATUS     deprecated
       DESCRIPTION
              "The deprecated group of objects providing for
               management of UDP over IPv4."
       ::= { udpMIBGroups 1 }

   udpBaseGroup OBJECT-GROUP
       OBJECTS   { udpInDatagrams, udpNoPorts, udpInErrors,
                   udpOutDatagrams }
       STATUS     current
       DESCRIPTION
              "The group of objects providing for counters of UDP
               statistics."
       ::= { udpMIBGroups 2 }

   udpHCGroup OBJECT-GROUP
       OBJECTS   { udpHCInDatagrams, udpHCOutDatagrams }
       STATUS     current
       DESCRIPTION
              "The group of objects providing for counters of high
               speed UDP implementations."
       ::= { udpMIBGroups 3 }

   udpEndpointGroup OBJECT-GROUP
       OBJECTS    { udpEndpointProcess }
       STATUS     current
       DESCRIPTION
              "The group of objects providing for the IP version
               independent management of UDP 'endpoints'."
       ::= { udpMIBGroups 4 }

   END
