

Printer-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Counter32, Integer32, TimeTicks,
        NOTIFICATION-TYPE, OBJECT-IDENTITY,
        mib-2 FROM SNMPv2-SMI                             -- [RFC2578]
    TEXTUAL-CONVENTION FROM SNMPv2-TC                     -- [RFC2579]
    MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
        FROM SNMPv2-CONF                                  -- [RFC2580]
    hrDeviceIndex, hrStorageIndex FROM HOST-RESOURCES-MIB -- [RFC2790]
    InterfaceIndexOrZero FROM IF-MIB                      -- [RFC2863]
    PrtCoverStatusTC, PrtGeneralResetTC, PrtChannelTypeTC,
        PrtInterpreterLangFamilyTC, PrtInputTypeTC, PrtOutputTypeTC,
        PrtMarkerMarkTechTC, PrtMarkerSuppliesTypeTC, PrtConsoleColorTC,
        PrtConsoleDisableTC, PrtMediaPathTypeTC, PrtAlertGroupTC,
        PrtAlertTrainingLevelTC, PrtAlertCodeTC
        FROM IANA-PRINTER-MIB
    IANACharset FROM IANA-CHARSET-MIB;

printmib MODULE-IDENTITY
    LAST-UPDATED "200406020000Z"
    ORGANIZATION "PWG IEEE/ISTO Printer Working Group"

    CONTACT-INFO
        "Harry Lewis
        IBM
        Phone (303) 924-5337
        Email: harryl@us.ibm.com
        http://www.pwg.org/index.html

        Send comments to the printmib WG using the Printer MIB
        Project (PMP) Mailing List:  pmp@pwg.org

        For further information, access the PWG web page under 'Printer
        MIB':      http://www.pwg.org/

        Implementers of this specification are encouraged to join the
        pmp mailing list in order to participate in discussions on any
        clarifications needed and registration proposals being reviewed
        in order to achieve consensus."
    DESCRIPTION
        "The MIB module for management of printers.
         Copyright (C) The Internet Society (2004). This
         version of this MIB module was published
         in RFC 3805. For full legal notices see the RFC itself."
    REVISION     "200406020000Z"
    DESCRIPTION
        "Printer MIB v2.
        Moved all enum groups to be maintained by IANA into new TCs
           within the ianaPrinterMIB, which is contained in this
           document.
        New TCs created from enums defined within RFC 1759 Objects:
           PrtPrintOrientationTC, PrtLocalizedDescriptionStringTC,
           PrtConsoleDescriptionStringTC, PrtChannelStateTC,
           PrtOutputStackingOrderTC, PrtOutputPageDeliveryOrientationTC,
           PrtMarkerCounterUnitTC, PrtMarkerSuppliesSupplyUnitTC,
           PrtMarkerSuppliesClassTC, PrtMarkerAddressabilityUnitTC,
           PrtMarkerColorantRoleTC, PrtMediaPathMaxSpeedPrintUnitTC,
           PrtInterpreterTwoWayTC, and PrtAlertSeverityLevelTC.
        The following four TCs have been deprecated:
           MediaUnit (replaced by PrtMediaUnitTC),
           CapacityUnit (replaced by PrtCapacityUnitTC),
           SubUnitStatus (replaced by PrtSubUnitStatusTC),
           CodedCharSet (replaced by IANACharset in IANA Charset MIB)
        Five new OBJECT-GROUPs: prtAuxilliarySheetGroup,
           prtInputSwitchingGroup, prtGeneralV2Group,
           prtAlertTableV2Group, prtChannelV2Group.
        Nine new objects added to those groups:
           prtAuxiliarySheetStartupPage, prtAuxiliarySheetBannerPage,
           prtGeneralPrinterName, prtGeneralSerialNumber,
           prtAlertCriticalEvents, prtAlertAllEvents,

           prtInputMediaLoadTimeout, prtInputNextIndex,
           prtChannelInformation.
        SYNTAX range changed from (0..65535) to (1..65535) for the
           index objects prtStorageRefSeqNumber, prtDeviceRefSeqNumber,
           and prtConsoleLightIndex.
        SYNTAX range changed from (0..65535) to (0..2147483647) for the
           objects prtStorageRefIndex and prtDeviceRefIndex to agree
           with the Host Resources MIB.
        Defined a range for the objects with a SYNTAX of Integer32:
           prtOutputDefaultIndex, prtInputMediaDimFeedDirDeclared,
           prtInputMediaDimXFeedDirDeclared, prtInputMaxCapacity,
           prtInputCurrentLevel, prtInputMediaDimFeedDirChosen,
           prtInputMediaDimXFeedDirChosen, prtInputMediaWeight,
           prtInputMediaFormParts, prtOutputIndex,
           prtOutputMaxCapacity, prtOutputRemainingCapacity,
           prtOutputMaxDimFeedDir, prtOutputMaxDimXFeedDir,
           prtOutputMinDimFeedDir, prtOutputMinDimXFeedDir,
           prtMarkerAddressibilityFeedDir,
           prtMarkerAddressibilityXFeedDir, prtMarkerNorthMargin,
           prtMarkerSouthMargin, prtMarkerWestMargin,
           prtMarkerEastMargin, prtMarkerSuppliesMaxCapacity,
           prtMarkerSuppliesLevel, prtMarkerColorantTonality,
           prtMediaPathMaxSpeed, prtMediaPathMaxMediaFeedDir,
           prtMediaPathMaxMediaXFeedDir, prtMediaPathMinMediaFeedDir,
           prtMediaPathMinMediaXFeedDir, prtChannelIndex,
           prtChannelCurrentJobCntlLangIndex, prtInterpreterIndex,
           prtChannelDefaultPageDescLangIndex, prtConsoleOnTime,
           prtInterpreterFeedAddressibility, prtConsoleOffTime,
           prtInterpreterXFeedAddressibility, prtAlertIndex,
           prtAlertGroupIndex, prtAlertLocation.
        Changed SYNTAX from Integer32 to InterfaceIndexOrZero for
           prtChannelIfIndex.
        Changed MAX-ACCESS of prtAlertIndex from not-accessible to
           Read-only and added a compliance statement to allow a
           MIN-ACCESS of accessible-for-notify.
        One new NOTIFICATION-GROUP: prtAlertTrapGroup which contains
           printerV2Alert.
        In MODULE-COMPLIANCE prtMIBCompliance, new OBJECT-GROUPs and
           the NOTIFICATION_GROUP, all in GROUP (not MANDATORY-GROUP)
           clauses.  The nine new objects are optional, i.e., this
           document is backward compatible with RFC 1759."
    REVISION     "199411250000Z"
    DESCRIPTION
        "The original version of this MIB, published as RFC1759."
    ::= { mib-2 43 }

-- TEXTUAL-CONVENTIONs for this MIB module
--
-- Generic unspecific TEXTUAL-CONVENTIONs
--

PrtMediaUnitTC ::= TEXTUAL-CONVENTION
    -- Replaces MediaUnit in RFC 1759.
    STATUS    current
    DESCRIPTION
        "Units of measure for media dimensions."
    SYNTAX    INTEGER {
                  tenThousandthsOfInches(3),  -- .0001
                  micrometers(4)
                  }

MediaUnit ::= TEXTUAL-CONVENTION
    -- Replaced by PrtMediaUnitTC.
    STATUS    deprecated
    DESCRIPTION
        "Units of measure for media dimensions."
    SYNTAX    INTEGER {
                  tenThousandthsOfInches(3),  -- .0001
                  micrometers(4)
                  }

PrtCapacityUnitTC ::= TEXTUAL-CONVENTION
    -- Replaces CapacityUnit in RFC 1759.
    STATUS    current
    DESCRIPTION
        "Units of measure for media capacity."
    SYNTAX    INTEGER {
                  other(1),                   -- New, not in RFC 1759
                  unknown(2),                 -- New, not in RFC 1759
                  tenThousandthsOfInches(3),  -- .0001
                  micrometers(4),
                  sheets(8),
                  feet(16),
                  meters(17),
                -- Values for Finisher MIB
                  items(18),                  -- New, not in RFC 1759
                  percent(19)                 -- New, not in RFC 1759
                  }

CapacityUnit ::= TEXTUAL-CONVENTION
    -- Replaced by PrtCapacityUnitTC.
    STATUS    deprecated
    DESCRIPTION
        "Units of measure for media capacity."

    SYNTAX    INTEGER {
                  tenThousandthsOfInches(3),  -- .0001
                  micrometers(4),
                  sheets(8),
                  feet(16),
                  meters(17)
                  }

PrtPrintOrientationTC ::= TEXTUAL-CONVENTION
    -- This TC was extracted from prtInterpreterDefaultOrientation in
    -- RFC 1759.
    STATUS    current
    DESCRIPTION
        "A generic representation for printing orientation on a
        'page'."
    SYNTAX    INTEGER {
                  other(1),
                  portrait(3),
                  landscape(4)
                  }

PrtSubUnitStatusTC ::= TEXTUAL-CONVENTION
    -- Replaces SubUnitStatus in RFC 1759.
    STATUS    current
    DESCRIPTION
        "Status of a printer sub-unit.

        The SubUnitStatus is an integer that is the sum of 5 distinct
        values, Availability, Non-Critical, Critical, On-line, and
        Transitioning. These values are:

        Availability                           Value

            Available and Idle                  0       0000'b
            Available and Standby               2       0010'b
            Available and Active                4       0100'b
            Available and Busy                  6       0110'b
            Unavailable and OnRequest           1       0001'b
            Unavailable because Broken          3       0011'b
            Unknown                             5       0101'b

        Non-Critical
            No Non-Critical Alerts              0       0000'b
            Non-Critical Alerts                 8       1000'b

        Critical

            No Critical Alerts                  0       0000'b

            Critical Alerts                    16     1 0000'b

        On-Line

            State is On-Line                    0       0000'b
            State is Off-Line                  32    10 0000'b

        Transitioning

            At intended state                   0       0000'b
            Transitioning to intended state    64   100 0000'b"

    SYNTAX    INTEGER (0..126)

SubUnitStatus ::= TEXTUAL-CONVENTION
   -- Replaced by PrtSubUnitStatusTC.
    STATUS    deprecated
    DESCRIPTION
        "Status of a printer sub-unit.

        The SubUnitStatus is an integer that is the sum of 5 distinct
        values, Availability, Non-Critical, Critical, On-line, and
        Transitioning. These values are:

        Availability                           Value
            Available and Idle                  0       0000'b
            Available and Standby               2       0010'b
            Available and Active                4       0100'b
            Available and Busy                  6       0110'b
            Unavailable and OnRequest           1       0001'b
            Unavailable because Broken          3       0011'b
            Unknown                             5       0101'b

        Non-Critical
            No Non-Critical Alerts              0       0000'b
            Non-Critical Alerts                 8       1000'b

        Critical

            No Critical Alerts                  0       0000'b
            Critical Alerts                    16     1 0000'b

        On-Line

            State is On-Line                    0       0000'b
            State is Off-Line                  32    10 0000'b

        Transitioning

            At intended state                   0       0000'b
            Transitioning to intended state    64   100 0000'b"

    SYNTAX    INTEGER (0..126)

PresentOnOff ::= TEXTUAL-CONVENTION
    STATUS    current
    DESCRIPTION
        "Presence and configuration of a device or feature."
    SYNTAX    INTEGER {
                  other(1),
                  on(3),
                  off(4),
                  notPresent(5)
                  }

PrtLocalizedDescriptionStringTC ::= TEXTUAL-CONVENTION
    -- This TC did not appear in RFC 1759.
    STATUS    current
    DESCRIPTION
        "An object MUST use this TEXTUAL-CONVENTION when its
        'charset' is controlled by the value of
        prtGeneralCurrentLocalization."
    SYNTAX    OCTET STRING (SIZE(0..255))

PrtConsoleDescriptionStringTC ::= TEXTUAL-CONVENTION
    -- This TC did not appear in RFC 1759.
    STATUS    current
    DESCRIPTION
        "An object MUST use this TEXTUAL-CONVENTION when its
        'charset' is controlled by the value of
        prtConsoleLocalization."
    SYNTAX    OCTET STRING (SIZE(0..255))

CodedCharSet ::= TEXTUAL-CONVENTION

   -- Replaced by IANACharset TEXTUAL-CONVENTION in IANA Charset MIB.
    STATUS     deprecated
    DESCRIPTION
       "The original description clause from RFC 1759 [RFC1759] was
       technically inaccurate and therefore has been deleted."
   SYNTAX     INTEGER {
     other(1)               -- used if the designated coded
                            -- character set is not currently in
                            -- the enumeration
}

--

-- Channel Group TEXTUAL-CONVENTIONs
--

PrtChannelStateTC ::= TEXTUAL-CONVENTION
    -- This TC was extracted from prtChannelState in RFC 1759.
    STATUS    current
    DESCRIPTION
        "The state of this print job delivery channel. The value
        determines whether print data is allowed through this channel."
    SYNTAX    INTEGER {
                  other(1),
                  printDataAccepted(3),
                  noDataAccepted(4)
                  }

--
-- Input/Output Group TEXTUAL-CONVENTIONs
--

PrtOutputStackingOrderTC ::= TEXTUAL-CONVENTION
    -- This TC was extracted from prtOutputStackingOrder in RFC 1759.
    STATUS    current
    DESCRIPTION
        "The current state of the stacking order for the associated
        output sub-unit. 'firstToLast' means that as pages are output,
        the front of the next page is placed against the back of the
        previous page. 'lastToFirst' means that as pages are output,
        the back of the next page is placed against the front of the
        previous page."
    SYNTAX    INTEGER {
                  unknown(2),
                  firstToLast(3),
                  lastToFirst(4)
                  }

PrtOutputPageDeliveryOrientationTC ::= TEXTUAL-CONVENTION
    -- This TC was extracted from prtOutputPageDeliveryOrientation
    -- in RFC 1759.
    STATUS    current
    DESCRIPTION
        "The reading surface that will be 'up' when pages are delivered
        to the associated output sub-unit. Values are Face-Up and Face
        Down (Note: interpretation of these values is, in general,
        context-dependent based on locale; presentation of these values
        to an end-user should be normalized to the expectations of the
        user."
    SYNTAX    INTEGER {
                  faceUp(3),

                  faceDown(4)
                  }

--
-- Marker Group TEXTUAL-CONVENTIONs
--

PrtMarkerCounterUnitTC ::= TEXTUAL-CONVENTION
    -- This TC was extracted from prtMarkerCounterUnit in RFC 1759.
    STATUS    current
    DESCRIPTION
        "The unit that will be used by the printer when reporting
        counter values for this marking sub-unit.  The
        time units of measure are provided for a device like a
        strip recorder that does not or cannot track the physical
        dimensions of the media and does not use characters,
        lines or sheets."

    SYNTAX    INTEGER {
                  tenThousandthsOfInches(3),  -- .0001
                  micrometers(4),
                  characters(5),
                  lines(6),
                  impressions(7),
                  sheets(8),
                  dotRow(9),
                  hours(11),
                  feet(16),
                  meters(17)
                  }

PrtMarkerSuppliesSupplyUnitTC ::= TEXTUAL-CONVENTION
    -- This TC was extracted from prtMarkerSuppliesSupplyUnit
    -- in RFC 1759.
    STATUS    current
    DESCRIPTION
        "Unit of this marker supply container/receptacle."
    SYNTAX    INTEGER {
                  other(1),                   -- New, not in RFC 1759
                  unknown(2),                 -- New, not in RFC 1759
                  tenThousandthsOfInches(3),  -- .0001
                  micrometers(4),
                  impressions(7),             -- New, not in RFC 1759
                  sheets(8),                  -- New, not in RFC 1759
                  hours(11),                  -- New, not in RFC 1759
                  thousandthsOfOunces(12),
                  tenthsOfGrams(13),
                  hundrethsOfFluidOunces(14),

                  tenthsOfMilliliters(15),
                  feet(16),                   -- New, not in RFC 1759
                  meters(17),                 -- New, not in RFC 1759
                -- Values for Finisher MIB
                  items(18),  -- e.g., #staples. New, not in RFC 1759
                  percent(19)                 -- New, not in RFC 1759
                  }

PrtMarkerSuppliesClassTC ::= TEXTUAL-CONVENTION
    -- This TC was extracted from prtMarkerSuppliesClass in RFC 1759.
    STATUS    current
    DESCRIPTION
        "Indicates whether this supply entity represents a supply
        that is consumed or a receptacle that is filled."
    SYNTAX    INTEGER {
                  other(1),
                  supplyThatIsConsumed(3),
                  receptacleThatIsFilled(4)
                  }

PrtMarkerColorantRoleTC ::= TEXTUAL-CONVENTION
    -- This TC was extracted from prtMarkerColorantRole in RFC 1759.
    STATUS    current
    DESCRIPTION
        "The role played by this colorant."
    SYNTAX    INTEGER { --  Colorant Role
                  other(1),
                  process(3),
                  spot(4)
                  }

PrtMarkerAddressabilityUnitTC ::= TEXTUAL-CONVENTION
    -- This TC was extracted from prtMarkerAddressabilityUnit
    -- in RFC 1759.
    STATUS    current
    DESCRIPTION
        "The unit of measure of distances, as applied to the marker's
        resolution."
    SYNTAX    INTEGER {
                  tenThousandthsOfInches(3), -- .0001
                  micrometers(4)
                  }

--
-- Media Path TEXTUAL-CONVENTIONs
--

PrtMediaPathMaxSpeedPrintUnitTC ::= TEXTUAL-CONVENTION

    -- This TC was extracted from prtMediaPathMaxSpeedPrintUnit
    -- in RFC 1759.
    STATUS    current
    DESCRIPTION
        "The unit of measure used in specifying the speed of all
        media paths in the printer."
    SYNTAX    INTEGER {
                  tenThousandthsOfInchesPerHour(3),-- .0001/hour
                  micrometersPerHour(4),
                  charactersPerHour(5),
                  linesPerHour(6),
                  impressionsPerHour(7),
                  sheetsPerHour(8),
                  dotRowPerHour(9),
                  feetPerHour(16),
                  metersPerHour(17)
                 }

--
-- Interpreter Group TEXTUAL-CONVENTIONs
--

PrtInterpreterTwoWayTC ::= TEXTUAL-CONVENTION
    -- This TC was extracted from prtInterpreterTwoWay in RFC 1759.
    STATUS    current
    DESCRIPTION
        "Indicates whether or not this interpreter returns information
        back to the host."
    SYNTAX    INTEGER {
                  yes(3),
                  no(4)
                  }

--
-- Alert Group TEXTUAL-CONVENTIONs
--

PrtAlertSeverityLevelTC ::= TEXTUAL-CONVENTION
    -- This TC was extracted from prtAlertSeverityLevel in RFC 1759.
    STATUS    current
    DESCRIPTION
        "The level of severity of this alert table entry.  The printer
        determines the severity level assigned to each entry in the
        table. A critical alert is binary by nature and definition. A
        warning is defined to be a non-critical alert. The original and
        most common warning is unary. The binary warning was added later
        and given a more distinguished name."
    SYNTAX    INTEGER {

                  other(1),
                  critical(3),
                  warning(4),
                  warningBinaryChangeEvent(5)   -- New, not in RFC 1759
                  }

-- The General Printer Group
--
-- The general printer sub-unit is responsible for the overall
-- control and status of the printer.  There is exactly one
-- general printer sub-unit in a printer.

prtGeneral OBJECT IDENTIFIER ::= { printmib 5 }

prtGeneralTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtGeneralEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of general information per printer.
        Objects in this table are defined in various
        places in the MIB, nearby the groups to
        which they apply.  They are all defined
        here to minimize the number of tables that would
        otherwise need to exist."
    ::= { prtGeneral 1 }

prtGeneralEntry OBJECT-TYPE
    SYNTAX     PrtGeneralEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "An entry exists in this table for each device entry in the
        host resources MIB device table with a device type of
        'printer'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX    { hrDeviceIndex }
    ::= { prtGeneralTable 1 }

PrtGeneralEntry ::= SEQUENCE {
    -- Note that not all of the objects in this sequence are in
    -- the general printer group. The group to which an
    -- object belongs is tagged with a label "General", "Input"
    -- "Output", etc. after each entry in the following sequence.
    --
    prtGeneralConfigChanges         Counter32, -- General

    prtGeneralCurrentLocalization   Integer32, -- General
    prtGeneralReset                 PrtGeneralResetTC,
                                               -- General
    prtGeneralCurrentOperator       OCTET STRING,
                                               -- Responsible Party
    prtGeneralServicePerson         OCTET STRING,
                                               -- Responsible Party
    prtInputDefaultIndex            Integer32, -- Input
    prtOutputDefaultIndex           Integer32, -- Output
    prtMarkerDefaultIndex           Integer32, -- Marker
    prtMediaPathDefaultIndex        Integer32, -- Media Path
    prtConsoleLocalization          Integer32, -- Console
    prtConsoleNumberOfDisplayLines  Integer32, -- Console
    prtConsoleNumberOfDisplayChars  Integer32, -- Console
    prtConsoleDisable               PrtConsoleDisableTC,
                                               -- Console,
    prtAuxiliarySheetStartupPage    PresentOnOff,
                                               -- AuxiliarySheet
    prtAuxiliarySheetBannerPage     PresentOnOff,
                                               -- AuxiliarySheet
    prtGeneralPrinterName           OCTET STRING,
                                               -- General V2
    prtGeneralSerialNumber          OCTET STRING,
                                               -- General V2
    prtAlertCriticalEvents          Counter32, -- Alert V2
    prtAlertAllEvents               Counter32  -- Alert V2
    }

prtGeneralConfigChanges OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Counts configuration changes within the printer. A
        configuration change is defined to be an action that results in
        a change to any MIB object other than those that reflect status
        or level, or those that act as counters or gauges. In addition,
        any action that results in a row being added or deleted from
        any table in the Printer MIB is considered a configuration
        change. Such changes will often affect the capability of the
        printer to service certain types of print jobs. Management
        applications may cache infrequently changed configuration
        information about sub units within the printer. This object
        should be incremented whenever the agent wishes to notify
        management applications that any cached configuration
        information for this device is to be considered 'stale'. At
        this point, the management application should flush any
        configuration information cached about this device and fetch

        new configuration information.

        The following are examples of actions that would cause the
        prtGeneralConfigChanges object to be incremented:

        - Adding an output bin
        - Changing the media in a sensing input tray
        - Changing the value of prtInputMediaType

        Note that the prtGeneralConfigChanges counter would not be
        incremented when an input tray is temporarily removed to load
        additional paper or when the level of an input device changes.

        NOTE: The above description has been modified from RFC 1759
        for clarification."

    ::= { prtGeneralEntry 1 }

prtGeneralCurrentLocalization OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of the prtLocalizationIndex corresponding to the
        current language, country, and character set to be used for
        localized string values that are identified as being dependent
        on the value of this object.  Note that this object does not
        apply to localized strings in the prtConsole group or to any
        object that is not explicitly identified as being localized
        according to prtGeneralCurrentLocalization.  When an object's
        'charset' is controlled by the value of
        prtGeneralCurrentLocalization, it MUST specify
        PrtLocalizedDescriptionStringTC as its syntax.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
   ::= { prtGeneralEntry 2 }

prtGeneralReset OBJECT-TYPE
    -- NOTE: In RFC 1759, the enumeration values were implicitly defined
    -- by this object.
    SYNTAX     PrtGeneralResetTC
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Setting this value to 'powerCycleReset', 'resetToNVRAM', or
        'resetToFactoryDefaults' will result in the resetting of the
        printer.  When read, this object will always have the value

        'notResetting(3)', and a SET of the value 'notResetting' shall
        have no effect on the printer.  Some of the defined values are
        optional.  However, every implementation must support at least
        the values 'notResetting' and 'resetToNVRAM'."
    ::= { prtGeneralEntry 3 }

-- The Responsible Party group

prtGeneralCurrentOperator OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..127))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The name of the person who is responsible for operating
        this printer.  It is suggested that this string include
        information that would enable other humans to reach the
        operator, such as a phone number.  As a convention to
        facilitate automatic notification of the operator by the
        agent or network management station, the phone number,
        fax number or email address should be indicated by the
        URL schemes 'tel:', 'fax:' and 'mailto:', respectively.
        If either the phone, fax, or email information is not
        available, then a line should not be included for this
        information.

        NOTE: For interoperability purposes, it is advisable to
        use email addresses formatted according to [RFC2822]
        requirements.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtGeneralEntry 4 }

prtGeneralServicePerson OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..127))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The name of the person responsible for servicing this
        printer.  It is suggested that this string include
        information that would enable other humans to reach the
        service person, such as a phone number.  As a convention
        to facilitate automatic notification of the operator by
        the agent or network management station, the phone
        number, fax number or email address should be indicated
        by the URL schemes 'tel:', 'fax:' and 'mailto:',
        respectively.  If either the phone, fax, or email
        information is not available, then a line should not

        be included for this information.

        NOTE: For interoperability purposes, it is advisable to use
        email addresses formatted per [RFC2822] requirements.

        NOTE: The above description has been modified from RFC 1759
        for clarification."

    ::= { prtGeneralEntry 5 }

-- Default indexes section
--
-- The following four objects are used to specify the indexes of
-- certain subunits used as defaults during the printing process.

prtInputDefaultIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of prtInputIndex corresponding to the default input
        sub-unit: that is, this object selects the default source of
        input media."
::= { prtGeneralEntry 6 }

prtOutputDefaultIndex OBJECT-TYPE
    --  A range has been added to the SYNTAX clause that was not in
    --  RFC 1759.  Although this violates SNMP compatibility rules,
    --  it provides a more reasonable guide for SNMP managers.
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of prtOutputIndex corresponding to the default
        output sub-unit; that is, this object selects the default
        output destination."
::= { prtGeneralEntry 7 }

prtMarkerDefaultIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of prtMarkerIndex corresponding to the
        default marker sub-unit; that is, this object selects the
        default marker."
    ::= { prtGeneralEntry 8 }

prtMediaPathDefaultIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of prtMediaPathIndex corresponding to
        the default media path; that is, the selection of the
        default media path."
    ::= { prtGeneralEntry 9 }

-- Console general section
--
-- The following four objects describe overall parameters of the
-- printer console subsystem.

prtConsoleLocalization OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of the prtLocalizationIndex corresponding to
        the language, country, and character set to be used for the
        console.  This localization applies both to the actual display
        on the console as well as the encoding of these console objects
        in management operations.  When an object's 'charset' is
        controlled by the value of prtConsoleLocalization, it MUST
        specify PrtConsoleDescriptionStringTC as its syntax.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtGeneralEntry 10 }

prtConsoleNumberOfDisplayLines OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The number of lines on the printer's physical
        display.  This value is 0 if there are no lines on the
        physical display or if there is no physical display"
    ::= { prtGeneralEntry 11 }

prtConsoleNumberOfDisplayChars OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The number of characters per line displayed on the physical

        display.  This value is 0 if there are no lines on the physical
        display or if there is no physical display"
    ::= { prtGeneralEntry 12 }

prtConsoleDisable OBJECT-TYPE
    -- In RFC 1759, the enumeration values were implicitly defined
    -- by this object.
    SYNTAX     PrtConsoleDisableTC
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This value indicates how input is (or is not) accepted from
        the operator console.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtGeneralEntry 13 }

-- The Auxiliary Sheet Group
--
-- The auxiliary sheet group allows the administrator to control
-- the production of auxiliary sheets by the printer.  This group
-- contains only the "prtAuxiliarySheetStartupPage" and
-- "prtAuxiliarySheetBannerPage" objects.

prtAuxiliarySheetStartupPage OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Used to enable or disable printing a startup page.  If enabled,
        a startup page will be printed shortly after power-up, when the
        device is ready.  Typical startup pages include test patterns
        and/or printer configuration information."
    ::= { prtGeneralEntry 14 }

prtAuxiliarySheetBannerPage OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Used to enable or disable printing banner pages at the
        beginning of jobs.  This is a master switch which applies to all
        jobs, regardless of interpreter."
     ::= { prtGeneralEntry 15 }

-- Administrative section  (The General V2 Group)
--
-- The following two objects are used to specify administrative
-- information assigned to the printer.

prtGeneralPrinterName OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..127))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "An administrator-specified name for this printer.  Depending
        upon implementation of this printer, the value of this object
        may or may not be same as the value for the MIB-II 'SysName'
        object."
     ::= { prtGeneralEntry 16 }

prtGeneralSerialNumber OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..255))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "A recorded serial number for this device that indexes some
        type device catalog or inventory.  This value is usually set by
        the device manufacturer but the MIB supports the option of
        writing for this object for site-specific administration of
        device inventory or tracking."
    ::= { prtGeneralEntry 17 }

-- General alert table section  (Alert Table V2 Group)
--
-- The following two objects are used to specify counters
-- associated with the Alert Table.

prtAlertCriticalEvents OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A running counter of the number of critical alert events that
        have been recorded in the alert table.  The value of this object
        is RESET in the event of a power cycle operation (i.e., the
        value is not persistent."
    ::= { prtGeneralEntry 18 }

prtAlertAllEvents OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current

    DESCRIPTION
        "A running counter of the total number of alert event entries
        (critical and non-critical) that have been recorded in the
        alert table"
    ::= { prtGeneralEntry 19 }

-- The Cover Table
--
-- The cover portion of the General print sub-unit describes the
-- covers and interlocks of the printer.  The Cover Table has an
-- entry for each cover and interlock.

prtCover OBJECT IDENTIFIER ::= { printmib 6 }

prtCoverTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtCoverEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of the covers and interlocks of the printer."
    ::= { prtCover 1 }

prtCoverEntry OBJECT-TYPE
    SYNTAX     PrtCoverEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Information about a cover or interlock.
        Entries may exist in the table for each device
        index with a device type of 'printer'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX  { hrDeviceIndex, prtCoverIndex }
    ::= { prtCoverTable 1 }

PrtCoverEntry ::= SEQUENCE {
    prtCoverIndex            Integer32,
    prtCoverDescription      PrtLocalizedDescriptionStringTC,
    prtCoverStatus           PrtCoverStatusTC
    }

prtCoverIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this Cover sub

        unit.  Although these values may change due to a major
        reconfiguration of the device (e.g., the addition of new cover
        sub-units to the printer), values SHOULD remain stable across
        successive printer power cycles.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtCoverEntry 1 }

prtCoverDescription OBJECT-TYPE
    -- In RFC 1759, the SYNTAX was OCTET STRING.  This has been changed
    -- to a TC to better support localization of the object.
    SYNTAX     PrtLocalizedDescriptionStringTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The manufacturer provided cover sub-mechanism name in the
        localization specified by prtGeneralCurrentLocalization."
    ::= { prtCoverEntry 2 }

prtCoverStatus  OBJECT-TYPE
    -- NOTE: In RFC 1759, the enumeration values were implicitly defined
    -- by this object and are now defined in the IANA-PRINTER-MIB.  The
    -- new TC has defined "coverOpen" and "coverClosed" to replace
    -- "doorOpen" and "doorClosed" in RFC 1759.  A name change is not
    -- formally allowed per SMI rules, but was agreed to by the WG group
    -- since a door has a more restrictive meaning than a cover and
    -- Cover group is intended to support doors as a subset of covers.

   SYNTAX     PrtCoverStatusTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The status of this cover sub-unit."
    ::= { prtCoverEntry 3 }

-- The Localization Table
--
-- The localization portion of the General printer sub-unit is
-- responsible for identifying the natural language, country, and
-- character set in which character strings are expressed.  There
-- may be one or more localizations supported per printer.  The
-- available localizations are represented by the Localization
-- table.

prtLocalization  OBJECT IDENTIFIER ::= { printmib 7 }

prtLocalizationTable OBJECT-TYPE

    SYNTAX     SEQUENCE OF PrtLocalizationEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The available localizations in this printer."
    ::= { prtLocalization 1 }

prtLocalizationEntry OBJECT-TYPE
    SYNTAX     PrtLocalizationEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A description of a localization.
        Entries may exist in the table for each device
        index with a device type of 'printer'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX  { hrDeviceIndex, prtLocalizationIndex }
    ::= { prtLocalizationTable 1 }

PrtLocalizationEntry ::= SEQUENCE {
    prtLocalizationIndex          Integer32,
    prtLocalizationLanguage       OCTET STRING,
    prtLocalizationCountry        OCTET STRING,
    prtLocalizationCharacterSet   IANACharset
    }

prtLocalizationIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this
        localization entry.  Although these values may change due to a
        major reconfiguration of the device (e.g., the addition of new
        localization data to the printer), values SHOULD remain
        stable across successive printer power cycles.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtLocalizationEntry 1 }

prtLocalizationLanguage OBJECT-TYPE
    -- Note: The size is fixed, was incorrectly 0..2 in RFC 1759.
    SYNTAX     OCTET STRING (SIZE(2))
    MAX-ACCESS read-only
    STATUS     current

    DESCRIPTION
        "A two character language code from ISO 639.  Examples en,
        es, fr, de.  NOTE: These examples were shown as upper case in
        RFC 1759 and are now shown as lower case to agree with ISO 639."
    ::= { prtLocalizationEntry 2 }

prtLocalizationCountry OBJECT-TYPE
    -- Note: The size is fixed, was incorrectly 0..2 in RFC 1759.
    SYNTAX     OCTET STRING (SIZE(2))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A two character country code from ISO 3166, a blank string
        (two space characters) shall indicate that the country is not
        defined.  Examples: US, GB, FR, DE, ..."
    ::= { prtLocalizationEntry 3 }

prtLocalizationCharacterSet OBJECT-TYPE
    SYNTAX     IANACharset
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
      "The coded character set used for this localization."
    ::= { prtLocalizationEntry 4 }

-- The System Resources Tables
--
-- The Printer MIB makes use of the Host Resources MIB to
-- define system resources by referencing the storage
-- and device groups of the print group.

prtStorageRefTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtStorageRefEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This table defines which printer, amongst multiple printers
        serviced by one agent, owns which storage units.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtGeneral 2 }

prtStorageRefEntry OBJECT-TYPE
    SYNTAX     PrtStorageRefEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION

        "This table will have an entry for each entry in the Host
        Resources MIB storage table that represents storage associated
        with a printer managed by this agent.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX      { hrStorageIndex, prtStorageRefSeqNumber }
    ::= { prtStorageRefTable 1 }

PrtStorageRefEntry ::= SEQUENCE {
    prtStorageRefSeqNumber  Integer32,
    prtStorageRefIndex      Integer32
    }

prtStorageRefSeqNumber OBJECT-TYPE
    -- NOTE: The range has been changed from RFC 1759, which allowed a
    -- minumum value of zero.  This was incorrect, since zero is not a
    -- valid index.
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This value will be unique amongst all entries with a common
        value of hrStorageIndex. This object allows a storage entry to
        point to the multiple printer devices with which it is
        associated."
    ::= { prtStorageRefEntry 1 }

prtStorageRefIndex OBJECT-TYPE
    -- NOTE: The range has been changed from RFC 1759 to be compatible
    -- with the defined range of hrDeviceIndex.
    SYNTAX     Integer32 (0..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The value of the hrDeviceIndex of the printer device that this
        storageEntry is associated with."
    ::= { prtStorageRefEntry 2 }

prtDeviceRefTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtDeviceRefEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This table defines which printer, amongst multiple printers
        serviced by one agent, is associated with which devices.

        NOTE: The above description has been modified from RFC 1759

        for clarification."
    ::= { prtGeneral 3 }

prtDeviceRefEntry OBJECT-TYPE
    SYNTAX     PrtDeviceRefEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This table will have an entry for each entry in the Host
        Resources MIB device table that represents a device associated
        with a printer managed by this agent.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX      { hrDeviceIndex, prtDeviceRefSeqNumber }
    ::= { prtDeviceRefTable 1 }

PrtDeviceRefEntry ::= SEQUENCE {
    prtDeviceRefSeqNumber   Integer32,
    prtDeviceRefIndex       Integer32
    }

prtDeviceRefSeqNumber OBJECT-TYPE
    -- NOTE: The range has been changed from RFC 1759, which allowed a
    -- minumum value of zero.  This was incorrect, since zero is not a
    -- valid index.
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This value will be unique amongst all entries with a common
        value of hrDeviceIndex. This object allows a device entry to
        point to the multiple printer devices with which it is
        associated."
    ::= { prtDeviceRefEntry 1 }

prtDeviceRefIndex OBJECT-TYPE
    -- NOTE: The range has been changed from RFC 1759 to be compatible
    -- with the defined range of hrDeviceIndex.
    SYNTAX     Integer32 (0..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The value of the hrDeviceIndex of the printer device that this
        deviceEntry is associated with."
    ::= { prtDeviceRefEntry 2 }

-- The Input Group
--
-- Input sub-units are managed as a tabular, indexed collection
-- of possible devices capable of providing media for input to
-- the printing process.  Input sub-units typically have a
-- location, a type, an identifier, a set of constraints on
-- possible media sizes and potentially other media
-- characteristics, and may be capable of indicating current
-- status or capacity.

prtInput   OBJECT IDENTIFIER ::= { printmib 8 }

prtInputTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtInputEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of the devices capable of providing media for input to
        the printing process."
    ::= { prtInput 2 }

prtInputEntry OBJECT-TYPE
    SYNTAX     PrtInputEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Attributes of a device capable of providing media for input to
        the printing process.  Entries may exist in the table for each
        device index with a device type of 'printer'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX  { hrDeviceIndex, prtInputIndex }
    ::= { prtInputTable 1 }

PrtInputEntry ::= SEQUENCE {
    prtInputIndex                     Integer32,
    prtInputType                      PrtInputTypeTC,
    prtInputDimUnit                   PrtMediaUnitTC,
    prtInputMediaDimFeedDirDeclared   Integer32,
    prtInputMediaDimXFeedDirDeclared  Integer32,
    prtInputMediaDimFeedDirChosen     Integer32,
    prtInputMediaDimXFeedDirChosen    Integer32,
    prtInputCapacityUnit              PrtCapacityUnitTC,
    prtInputMaxCapacity               Integer32,
    prtInputCurrentLevel              Integer32,
    prtInputStatus                    PrtSubUnitStatusTC,
    prtInputMediaName                 OCTET STRING,

    prtInputName                      OCTET STRING,
    prtInputVendorName                OCTET STRING,
    prtInputModel                     OCTET STRING,
    prtInputVersion                   OCTET STRING,
    prtInputSerialNumber              OCTET STRING,
    prtInputDescription               PrtLocalizedDescriptionStringTC,
    prtInputSecurity                  PresentOnOff,
    prtInputMediaWeight               Integer32,
    prtInputMediaType                 OCTET STRING,
    prtInputMediaColor                OCTET STRING,
    prtInputMediaFormParts            Integer32,
    prtInputMediaLoadTimeout          Integer32,
    prtInputNextIndex                 Integer32
    }

prtInputIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this input
        sub-unit.  Although these values may change due to a major
        reconfiguration of the device (e.g., the addition of new input
        sub-units to the printer), values SHOULD remain stable across
        successive printer power cycles.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtInputEntry 1 }

prtInputType OBJECT-TYPE
    -- NOTE: In RFC 1759, the enumeration values were implicitly
    -- defined by this object.
    SYNTAX     PrtInputTypeTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The type of technology (discriminated primarily according to
        feeder mechanism type) employed by the input sub-unit.  Note,
        the Input Class provides for a descriptor field to further
        qualify the other choice."
    ::= { prtInputEntry 2 }

prtInputDimUnit OBJECT-TYPE
    SYNTAX     PrtMediaUnitTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION

        "The unit of measurement for use calculating and relaying
         dimensional values for this input sub-unit."
    ::= { prtInputEntry 3 }

prtInputMediaDimFeedDirDeclared OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This object provides the value of the declared dimension, in
        the feed direction, of the media that is (or, if empty, was or
        will be) in this input sub-unit.  The feed direction is the
        direction in which the media is fed on this sub-unit.  This
        dimension is measured in input sub-unit dimensional units
        (controlled by prtInputDimUnit, which uses PrtMediaUnitTC).  If
        this input sub-unit can reliably sense this value, the value is
        sensed by the printer and may not be changed by management
        requests.  Otherwise, the value may be changed.  The value (-1)
        means other and specifically means that this sub-unit places no
        restriction on this parameter.  The value (-2) indicates
        unknown."
    ::= { prtInputEntry 4 }

prtInputMediaDimXFeedDirDeclared OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This object provides the value of the declared dimension, in
        the cross feed direction, of the media that is (or, if empty,
        was or will be) in this input sub-unit.  The cross  feed
        direction is ninety degrees relative to the feed direction
        associated with this sub-unit.  This dimension is measured in
        input sub-unit dimensional units (controlled by
        prtInputDimUnit,which uses PrtMediaUnitTC).  If this input sub-
        unit can reliably sense this value, the value is sensed by the
        printer and may not be changed by management requests.
        Otherwise, the value may be changed.  The value (-1) means other
        and specifically means that this sub-unit places no restriction
        on this parameter.  The value (-2) indicates unknown."
    ::= { prtInputEntry 5 }

prtInputMediaDimFeedDirChosen OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only

    STATUS     current
    DESCRIPTION
        "The printer will act as if media of the chosen dimension (in
        the feed direction) is present in this input source.  Note that
        this value will be used even if the input tray is empty.  Feed
        dimension measurements are taken relative to the feed direction
        associated with that sub-unit and are in input sub-unit
        dimensional units (controlled by prtInputDimUnit, which uses
        PrtMediaUnitTC).  If the printer supports the declared
        dimension,the granted dimension is the same as the declared
        dimension.  If not, the granted dimension is set to the closest
        dimension that the printer supports when the declared dimension
        is set.  The value (-1) means other and specifically indicates
        that this sub-unit places no restriction on this parameter.  The
        value (-2)indicates unknown."
    ::= { prtInputEntry 6 }

prtInputMediaDimXFeedDirChosen OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The printer will act as if media of the chosen dimension (in
        the cross feed direction) is present in this input source.  Note
        that this value will be used even if the input tray is empty.
        The cross feed direction is ninety degrees relative to the feed
        direction associated with this sub-unit.  This dimension is
        measured in input sub-unit dimensional units (controlled by
        prtInputDimUnit, which uses PrtMediaUnitTC).  If the printer
        supports the declare dimension, the granted dimension is the
        same as the declared dimension.  If not, the granted dimension
        is set to the closest dimension that the printer supports when
        the declared dimension is set.  The value (-1) means other and
        specifically indicates that this sub-unit places no restriction
        on this parameter.  The value (-2) indicates unknown."
    ::= { prtInputEntry 7 }

prtInputCapacityUnit OBJECT-TYPE
    -- NOTE: In RFC 1759, the enumeration values were implicitly
    -- defined by this object.
    SYNTAX     PrtCapacityUnitTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The unit of measurement for use in calculating and relaying
        capacity values for this input sub-unit."
    ::= { prtInputEntry 8 }

prtInputMaxCapacity OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The maximum capacity of the input sub-unit in input sub-unit
        capacity units (PrtCapacityUnitTC).  There is no convention
        associated with the media itself so this value reflects claimed
        capacity.  If this input sub-unit can reliably sense this value,
        the value is sensed by the printer and may not be changed by
        management requests; otherwise, the value may be written (by a
        Remote Control Panel or a Management Application). The value
        (-1) means other and specifically indicates that the sub-unit
        places no restrictions on this parameter.  The value (-2) means
        unknown."
    ::= { prtInputEntry 9 }

prtInputCurrentLevel OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-3..2147483647)    -- in capacity units
                                             -- (PrtCapacityUnitTC).
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The current capacity of the input sub-unit in input sub-unit
        capacity units (PrtCapacityUnitTC).  If this input sub-unit can
        reliably sense this value, the value is sensed by the printer
        and may not be changed by management requests; otherwise, the
        value may be written (by a Remote Control Panel or a Management
        Application).  The value (-1) means other and specifically
        indicates that the sub-unit places no restrictions on this
        parameter.  The value (-2) means unknown.  The value (-3) means
        that the printer knows that at least one unit remains."
    ::= { prtInputEntry 10 }

prtInputStatus OBJECT-TYPE
    SYNTAX     PrtSubUnitStatusTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The current status of this input sub-unit."
    ::= { prtInputEntry 11 }

prtInputMediaName OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-write
    STATUS     current

    DESCRIPTION
        "A description of the media contained in this input sub-unit;
        This description is to be used by a client to format and
        Localize a string for display to a human operator.  This
        description is not processed by the printer.  It is used to
        provide information not expressible in terms of the other
        media attributes (e.g., prtInputMediaDimFeedDirChosen,
        prtInputMediaDimXFeedDirChosen, prtInputMediaWeight,
        prtInputMediaType)."
    -- The following reference was not included in RFC 1759.
    REFERENCE
         "The PWG Standardized Media Names specification [PWGMEDIA]
         contains the recommended values for this object.  See also
         RFC 3805 Appendix C,'Media Names', which lists the values
         Of standardized media names defined in ISO/IEC 10175."
    ::= { prtInputEntry 12 }

--             INPUT MEASUREMENT
--
--     _______ |               |
--      ^      |               |
--      |      |               |                 |
--      |      |_ _ _ _ _ _ _ _| _______________ |direction
--      |      |               |      ^          v
-- MaxCapacity |    Sheets     |      |
--      |      |     left      | CurrentLevel
--      |      |      in       |      |
--      v      |     tray      |      v
--     _______ +_______________+ _______

-- The Extended Input Group

prtInputName OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The name assigned to this input sub-unit."
    ::= { prtInputEntry 13 }

prtInputVendorName OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The vendor name of this input sub-unit."
    ::= { prtInputEntry 14 }

prtInputModel OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The model name of this input sub-unit."
    ::= { prtInputEntry 15 }

prtInputVersion OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The version of this input sub-unit."
    ::= { prtInputEntry 16 }

prtInputSerialNumber OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..32))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The serial number assigned to this input sub-unit."
    ::= { prtInputEntry 17 }

prtInputDescription OBJECT-TYPE
    -- In RFC 1759, the SYNTAX was OCTET STRING.  This has been changed
    -- to a TC to better support localization of the object.
    SYNTAX     PrtLocalizedDescriptionStringTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A free-form text description of this input sub-unit in the
        localization specified by  prtGeneralCurrentLocalization."
    ::= { prtInputEntry 18 }

prtInputSecurity OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Indicates if this input sub-unit has some security associated
        with it."
    ::= { prtInputEntry 19 }

-- The Input Media Group
--
-- The Input Media Group supports identification of media
-- installed or available for use on a printing device.

-- Medium resources are identified by name, and include a
-- collection of characteristic attributes that may further be
-- used for selection and management of them.
-- The Input Media group consists of a set of optional
-- "columns" in the Input Table.  In this manner, a minimally
-- conforming implementation may choose to not support reporting
-- of media resources if it cannot do so.

prtInputMediaWeight  OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The weight of the medium associated with this input sub-unit
        in grams / per meter squared.  The value (-2) means unknown."
    ::= { prtInputEntry 20 }

prtInputMediaType OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The name of the type of medium associated with this input sub
        unit.  This name need not be processed by the printer; it might
        simply be displayed to an operator.

        NOTE: The above description has been modified from RFC 1759."
    -- The following reference was not included in RFC 1759.
    REFERENCE
        "The PWG Standardized Media Names specification [PWGMEDIA],
        section 3 Media Type Names, contains the recommended values for
        this object.  Implementers may add additional string values.
        The naming conventions in ISO 9070 are recommended in order to
        avoid potential name clashes."
    ::= { prtInputEntry 21 }

prtInputMediaColor OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The name of the color of the medium associated with
        this input sub-unit using standardized string values.

        NOTE: The above description has been modified from RFC 1759."
    -- The following reference was not included in RFC 1759.
    REFERENCE

        "The PWG Standardized Media Names specification [PWGMEDIA],
        section 4 Media Color Names, contains the recommended values
        for this object.  Implementers may add additional string values.
        The naming conventions in ISO 9070 are recommended in order to
        avoid potential name clashes."
    ::= { prtInputEntry 22 }

prtInputMediaFormParts OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The number of parts associated with the medium
        associated with this input sub-unit if the medium is a
        multi-part form.  The value (-1) means other and
        specifically indicates that the device places no
        restrictions on this parameter.  The value (-2) means
        unknown."
    ::= { prtInputEntry 23 }

-- The Input Switching Group
--
-- The input switching group allows the administrator to set the
-- input subunit time-out for the printer and to control the
-- automatic input subunit switching by the printer when an input
-- subunit becomes empty.

prtInputMediaLoadTimeout OBJECT-TYPE
   SYNTAX     Integer32 (-2..2147483647)
   MAX-ACCESS read-write
   STATUS     current
   DESCRIPTION
        "When the printer is not able to print due to a subunit being
        empty or the requested media must be manually loaded, the
        printer will wait for the duration (in seconds) specified by
        this object.  Upon expiration of the time-out, the printer will
        take the action specified by prtInputNextIndex.

        The event which causes the printer to enter the waiting state
        is product specific.  If the printer is not waiting for manually
        fed media, it may switch from an empty subunit to a different
        subunit without waiting for the time-out to expire.

        A value of (-1) implies 'other' or 'infinite' which translates
        to 'wait forever'.  The action which causes printing to continue
        is product specific.  A value of (-2) implies 'unknown'."
   ::= { prtInputEntry 24 }

prtInputNextIndex OBJECT-TYPE
   SYNTAX     Integer32 (-3..2147483647)
   MAX-ACCESS read-write
   STATUS     current
   DESCRIPTION
        "The value of prtInputIndex corresponding to the input subunit
        which will be used when this input subunit is emptied and the
        time-out specified by prtInputMediaLoadTimeout expires.  A value
        of zero(0) indicates that auto input switching will not occur
        when this input subunit is emptied.  If the time-out specified
        by prtInputLoadMediaTimeout expires and this value is zero(0),
        the job will be aborted.  A value of (-1) means other.  The
        value (-2)means 'unknown' and specifically indicates that an
        implementation specific method will determine the next input
        subunit to use at the time this subunit is emptied and the time
        out expires.  The value(-3) means input switching is not
        supported for this subunit."
   ::= { prtInputEntry 25 }

-- The Output Group
--
-- Output sub-units are managed as a tabular, indexed collection
-- of possible devices capable of receiving media delivered from
-- the printing process.  Output sub-units typically have a
-- location, a type, an identifier, a set of constraints on
-- possible media sizes and potentially other characteristics,
-- and may be capable of indicating current status or capacity.

prtOutput  OBJECT IDENTIFIER ::= { printmib 9 }

prtOutputTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtOutputEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of the devices capable of receiving media delivered
        from the printing process."
    ::= { prtOutput 2 }

prtOutputEntry OBJECT-TYPE
    SYNTAX     PrtOutputEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Attributes of a device capable of receiving media delivered
        from the printing process.  Entries may exist in the table for
        each device index with a device type of 'printer'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
   INDEX  { hrDeviceIndex, prtOutputIndex }
    ::= { prtOutputTable 1 }

PrtOutputEntry ::= SEQUENCE {
    prtOutputIndex                    Integer32,
    prtOutputType                     PrtOutputTypeTC,
    prtOutputCapacityUnit             PrtCapacityUnitTC,
    prtOutputMaxCapacity              Integer32,
    prtOutputRemainingCapacity        Integer32,
    prtOutputStatus                   PrtSubUnitStatusTC,
    prtOutputName                     OCTET STRING,
    prtOutputVendorName               OCTET STRING,
    prtOutputModel                    OCTET STRING,
    prtOutputVersion                  OCTET STRING,
    prtOutputSerialNumber             OCTET STRING,
    prtOutputDescription              PrtLocalizedDescriptionStringTC,
    prtOutputSecurity                 PresentOnOff,
    prtOutputDimUnit                  PrtMediaUnitTC,
    prtOutputMaxDimFeedDir            Integer32,
    prtOutputMaxDimXFeedDir           Integer32,
    prtOutputMinDimFeedDir            Integer32,
    prtOutputMinDimXFeedDir           Integer32,
    prtOutputStackingOrder        PrtOutputStackingOrderTC,
    prtOutputPageDeliveryOrientation
                        PrtOutputPageDeliveryOrientationTC,
    prtOutputBursting                 PresentOnOff,
    prtOutputDecollating              PresentOnOff,
    prtOutputPageCollated             PresentOnOff,
    prtOutputOffsetStacking           PresentOnOff
    }

prtOutputIndex OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by this printer to identify this output
        sub-unit.  Although these values may change due to a major
        reconfiguration of the sub-unit (e.g., the addition of new
        output devices to the printer), values SHOULD remain stable
        across successive printer power cycles.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtOutputEntry 1 }

prtOutputType OBJECT-TYPE
    -- NOTE: In RFC 1759, the enumeration values were implicitly defined
    -- by this object.
    SYNTAX     PrtOutputTypeTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The type of technology supported by this output sub-unit."
    ::= { prtOutputEntry 2 }

prtOutputCapacityUnit OBJECT-TYPE
    SYNTAX     PrtCapacityUnitTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The unit of measurement for use in calculating and relaying
        capacity values for this output sub-unit."
    ::= { prtOutputEntry 3 }

prtOutputMaxCapacity OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The maximum capacity of this output sub-unit in output sub-
        unit capacity units (PrtCapacityUnitTC).  There is no convention
        associated with the media itself so this value essentially
        reflects claimed capacity.  If this output sub-unit can reliably
        sense this value, the value is sensed by the printer and may
        not be changed by management requests; otherwise, the value may
        be written (by a Remote Control Panel or a Management
        Application).  The value (-1) means other and specifically
        indicates that the sub-unit places no restrictions on this
        parameter.  The value (-2) means unknown."
    ::= { prtOutputEntry 4 }

prtOutputRemainingCapacity OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-3..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The remaining capacity of the possible output sub-unit
        capacity in output sub-unit capacity units
        (PrtCapacityUnitTC)of this output sub-unit.  If this output sub-
        unit can reliably sense this value, the value is sensed by the
        printer and may not be modified by management requests;

        otherwise, the value may be written (by a Remote Control Panel
        or a Management Application).  The value (-1) means other and
        specifically indicates that the sub-unit places no restrictions
        on this parameter.  The value (-2) means unknown.  The value
        (-3) means that the printer knows that there remains capacity
        for at least one unit."
    ::= { prtOutputEntry 5 }

prtOutputStatus OBJECT-TYPE
    SYNTAX     PrtSubUnitStatusTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The current status of this output sub-unit."
    ::= { prtOutputEntry 6 }

--            OUTPUT MEASUREMENT
--
--   _______  |                | ________
--      ^     |                |     ^
--      |     |                |     |
--      |     |                |RemainingCapacity
-- MaxCapacity|                |     |
--      |     |                |     v           ^
--      |     |_ _ _ _ _ _ _ _ | _______________ |direction
--      |     |    Sheets      |                 |
--      |     |      in        |
--      v     |    Output      |
--   _______  +________________+

-- The Extended Output Group

prtOutputName OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The name assigned to this output sub-unit."
    ::= { prtOutputEntry 7 }

prtOutputVendorName OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The vendor name of this output sub-unit."
    ::= { prtOutputEntry 8 }

prtOutputModel OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The model name assigned to this output sub-unit.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtOutputEntry 9 }

prtOutputVersion OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The version of this output sub-unit."
    ::= { prtOutputEntry 10 }

prtOutputSerialNumber OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The serial number assigned to this output sub-unit."
    ::= { prtOutputEntry 11 }

prtOutputDescription OBJECT-TYPE
    -- In RFC 1759, the SYNTAX was OCTET STRING.  This has been changed
    -- to a TC to better support localization of the object.
    SYNTAX     PrtLocalizedDescriptionStringTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A free-form text description of this output sub-unit in the
        localization specified by prtGeneralCurrentLocalization."
    ::= { prtOutputEntry 12 }

prtOutputSecurity OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Indicates if this output sub-unit has some security associated
        with it and if that security is enabled or not."
    ::= { prtOutputEntry 13 }

-- The Output Dimensions Group

prtOutputDimUnit OBJECT-TYPE
    SYNTAX     PrtMediaUnitTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The unit of measurement for use in calculating and relaying
        dimensional values for this output sub-unit."
    ::= { prtOutputEntry 14 }

prtOutputMaxDimFeedDir OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The maximum dimensions supported by this output sub-unit
        for measurements taken parallel relative to the feed
        direction associated with that sub-unit in output
        sub-unit dimensional units (controlled by prtOutputDimUnit,
        which uses PrtMediaUnitTC).  If this output sub-unit can
        reliably sense this value, the value is sensed by the printer
        and may not be changed with management protocol operations.
        The value (-1) means other and specifically indicates that the
        sub-unit places no restrictions on this parameter.  The value
        (-2) means unknown.

        NOTE: The above description has been modified from RFC 1759
        for clarification and to explain the purpose of (-1) and (-2)."
    ::= { prtOutputEntry 15 }

prtOutputMaxDimXFeedDir OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The maximum dimensions supported by this output sub-unit
        for measurements taken ninety degrees relative to the
        feed direction associated with that sub-unit in output
        sub-unit dimensional units (controlled by prtOutputDimUnit,
        which uses PrtMediaUnitTC).  If this output sub-unit can
        reliably sense this value, the value is sensed by the printer
        and may not be changed with management protocol operations.
        The value (-1) means other and specifically indicates that the
        sub-unit places no restrictions on this parameter.  The value
        (-2) means unknown.

        NOTE: The above description has been modified from RFC 1759
        for clarification and to explain the purpose of (-1) and (-2)."
    ::= { prtOutputEntry 16 }

prtOutputMinDimFeedDir OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The minimum dimensions supported by this output sub-unit
        for measurements taken parallel relative to the feed
        direction associated with that sub-unit in output
        sub-unit dimensional units (controlled by prtOutputDimUnit,
        which uses PrtMediaUnitTC).  If this output sub-unit can
        reliably sense this value, the value is sensed by the printer
        and may not be changed with management protocol operations.
        The value (-1) means other and specifically indicates that the
        sub-unit places no restrictions on this parameter.  The value
        (-2) means unknown.

        NOTE: The above description has been modified from RFC 1759
        for clarification and to explain the purpose of (-1) and (-2)."
    ::= { prtOutputEntry 17 }

prtOutputMinDimXFeedDir OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The minimum dimensions supported by this output sub-unit
        for measurements taken ninety degrees relative to the
        feed direction associated with that sub-unit in output
        sub-unit dimensional units (controlled by prtOutputDimUnit,
        which uses PrtMediaUnitTC).  If this output sub-unit can
        reliably sense this value, the value is sensed by the printer
        and may not be changed with management protocol operations.
        The value (-1) means other and specifically indicates that the
        sub-unit places no restrictions on this parameter.  The value
        (-2) means unknown.

        NOTE: The above description has been modified from RFC 1759
        for clarification and to explain the purpose of (-1) and (-2)."
    ::= { prtOutputEntry 18 }

-- The Output Features Group

prtOutputStackingOrder OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtOutputStackingOrderTC
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The current state of the stacking order for the
        associated output sub-unit. 'FirstToLast' means
        that as pages are output the front of the next page is
        placed against the back of the previous page.
        'LasttoFirst' means that as pages are output the back
        of the next page is placed against the front of the
        previous page."
    ::= { prtOutputEntry 19 }

prtOutputPageDeliveryOrientation OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtOutputPageDeliveryOrientationTC
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The reading surface that will be 'up' when pages are
        delivered to the associated output sub-unit.  Values are
        faceUp and faceDown.  (Note: interpretation of these
        values is in general context-dependent based on locale;
        presentation of these values to an end-user should be
        normalized to the expectations of the user)."
    ::= { prtOutputEntry 20 }

prtOutputBursting OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This object indicates that the outputting sub-unit supports
        bursting, and if so, whether the feature is enabled.  Bursting
        is the process by which continuous media is separated into
        individual sheets, typically by bursting along pre-formed
        perforations."
    ::= { prtOutputEntry 21 }

prtOutputDecollating OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write

    STATUS     current
    DESCRIPTION
        "This object indicates that the output supports decollating,
        and if so, whether the feature is enabled.  Decollating is the
        process by which the individual parts within a multi-part form
        are separated and sorted into separate stacks for each part."
    ::= { prtOutputEntry 22 }

prtOutputPageCollated OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This object indicates that the output sub-unit supports page
        collation, and if so, whether the feature is enabled.  See RFC
        3805 Appendix A, Glossary Of Terms, for definition of how this
        document defines collation.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtOutputEntry 23 }

prtOutputOffsetStacking OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This object indicates that the output supports offset
        stacking,and if so, whether the feature is enabled.  See RFC
        3805 Appendix A, Glossary Of Terms,  for how Offset Stacking is
        defined by this document.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtOutputEntry 24 }

-- The Marker Group
--
-- A marker is the mechanism that produces marks on the print
-- media.  The marker sub-units and their associated supplies are
-- represented by the Marker Group in the model.  A printer can
-- contain one or more marking mechanisms.  Some examples of
-- multiple marker sub-units are: a printer
-- with separate markers for normal and magnetic ink or an
-- imagesetter that can output to both a proofing device and
-- final film.  Each marking device can have its own set of
-- characteristics associated with it, such as marking technology
-- and resolution.

prtMarker OBJECT IDENTIFIER ::= { printmib 10 }

-- The printable area margins as listed below define an area of
-- the print media which is guaranteed to be printable for all
-- combinations of input, media paths, and interpreters for this
-- marker.

prtMarkerTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtMarkerEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The marker table provides a description of each marker
        sub-unit contained within the printer.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMarker 2 }

prtMarkerEntry OBJECT-TYPE
    SYNTAX     PrtMarkerEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Entries in this table define the characteristics and status
        of each marker sub-unit in the printer.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX  { hrDeviceIndex, prtMarkerIndex }
    ::= { prtMarkerTable 1 }

PrtMarkerEntry ::= SEQUENCE {
    prtMarkerIndex                  Integer32,
    prtMarkerMarkTech               PrtMarkerMarkTechTC,
    prtMarkerCounterUnit            PrtMarkerCounterUnitTC,
    prtMarkerLifeCount              Counter32,
    prtMarkerPowerOnCount           Counter32,
    prtMarkerProcessColorants       Integer32,
    prtMarkerSpotColorants          Integer32,
    prtMarkerAddressabilityUnit     PrtMarkerAddressabilityUnitTC,
    prtMarkerAddressabilityFeedDir  Integer32,
    prtMarkerAddressabilityXFeedDir Integer32,
    prtMarkerNorthMargin            Integer32,
    prtMarkerSouthMargin            Integer32,
    prtMarkerWestMargin             Integer32,
    prtMarkerEastMargin             Integer32,
    prtMarkerStatus                 PrtSubUnitStatusTC

    }

prtMarkerIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this marking
        SubUnit.  Although these values may change due to a major
        reconfiguration of the device (e.g., the addition of new marking
        sub-units to the printer), values SHOULD remain stable across
        successive printer power cycles.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMarkerEntry 1 }

prtMarkerMarkTech OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtMarkerMarkTechTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The type of marking technology used for this marking
        sub-unit."
    ::= { prtMarkerEntry 2 }

prtMarkerCounterUnit OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtMarkerCounterUnitTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The unit that will be used by the printer when reporting
        counter values for this marking sub-unit.  The time units of
        measure are provided for a device like a strip recorder that
        does not or cannot track the physical dimensions of the media
        and does not use characters, lines or sheets."
    ::= { prtMarkerEntry 3 }

prtMarkerLifeCount OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The count of the number of units of measure counted during the

        life of printer using units of measure as specified by
        prtMarkerCounterUnit.

        Note: This object should be implemented as a persistent object
        with a reliable value throughout the lifetime of the printer."
    ::= { prtMarkerEntry 4 }

prtMarkerPowerOnCount OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The count of the number of units of measure counted since the
        equipment was most recently powered on using units of measure
        as specified by prtMarkerCounterUnit."
    ::= { prtMarkerEntry 5 }

prtMarkerProcessColorants OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The number of process colors supported by this marker.  A
        process color of 1 implies monochrome.  The value of this
        object and prtMarkerSpotColorants cannot both be 0.  The value
        of prtMarkerProcessColorants must be 0 or greater.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMarkerEntry 6 }

prtMarkerSpotColorants OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The number of spot colors supported by this marker.  The value
        of this object and prtMarkerProcessColorants cannot both be 0.
        Must be 0 or greater.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMarkerEntry 7 }

prtMarkerAddressabilityUnit OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtMarkerAddressabilityUnitTC

    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The unit of measure of distances, as applied to the marker's
        resolution.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMarkerEntry 8 }

prtMarkerAddressabilityFeedDir OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The maximum number of addressable marking positions in the
        feed direction per 10000 units of measure specified by
        prtMarkerAddressabilityUnit.  A value of (-1) implies 'other'
        or 'infinite' while a value of (-2) implies 'unknown'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMarkerEntry 9 }

prtMarkerAddressabilityXFeedDir OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The maximum number of addressable marking positions in the
        cross feed direction in 10000 units of measure specified by
        prtMarkerAddressabilityUnit.  A value of (-1) implies 'other'
        or 'infinite' while a value of (-2) implies 'unknown'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMarkerEntry 10 }

prtMarkerNorthMargin OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The margin, in units identified by prtMarkerAddressabilityUnit,
        from the leading edge of the medium as the medium flows through

        the marking engine with the side to be imaged facing the
        observer.  The leading edge is the North edge and the other
        edges are defined by the normal compass layout of  directions
        with the compass facing the observer.  Printing within the area
        bounded by all four margins is guaranteed for all interpreters.
        The value (-2) means unknown."
    ::= { prtMarkerEntry 11 }

prtMarkerSouthMargin OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The margin from the South edge  (see prtMarkerNorthMargin) of
        the medium in units identified by prtMarkerAddressabilityUnit.
        Printing within the area bounded by all four margins  is
        guaranteed for all interpreters.  The value (-2) means unknown."
    ::= { prtMarkerEntry 12 }

prtMarkerWestMargin OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The margin from the West edge (see prtMarkerNorthMargin) of
        the medium in units identified by prtMarkerAddressabilityUnit.
        Printing within the area bounded by all four margins is
        guaranteed for all interpreters.  The value (-2) means unknown."
    ::= { prtMarkerEntry 13 }

prtMarkerEastMargin OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The margin from the East edge (see prtMarkerNorthMargin) of
        the medium in units identified by prtMarkerAddressabilityUnit.
        Printing within the area bounded by all four margins is
        guaranteed for all interpreters.  The value (-2) means unknown."
    ::= { prtMarkerEntry 14 }

prtMarkerStatus OBJECT-TYPE
    SYNTAX     PrtSubUnitStatusTC
    MAX-ACCESS read-only
    STATUS     current

    DESCRIPTION
        "The current status of this marker sub-unit."
    ::= { prtMarkerEntry 15 }

-- The Marker Supplies Group

prtMarkerSupplies OBJECT IDENTIFIER ::= { printmib 11 }

prtMarkerSuppliesTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtMarkerSuppliesEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of the marker supplies available on this printer."
    ::= { prtMarkerSupplies 1 }

prtMarkerSuppliesEntry OBJECT-TYPE
    SYNTAX     PrtMarkerSuppliesEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Attributes of a marker supply.  Entries may exist in the table
        for each device index with a device type of 'printer'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX  { hrDeviceIndex, prtMarkerSuppliesIndex }
    ::= { prtMarkerSuppliesTable 1 }
PrtMarkerSuppliesEntry ::= SEQUENCE {
    prtMarkerSuppliesIndex          Integer32,
    prtMarkerSuppliesMarkerIndex    Integer32,
    prtMarkerSuppliesColorantIndex  Integer32,
    prtMarkerSuppliesClass          PrtMarkerSuppliesClassTC,
    prtMarkerSuppliesType           PrtMarkerSuppliesTypeTC,
    prtMarkerSuppliesDescription    PrtLocalizedDescriptionStringTC,
    prtMarkerSuppliesSupplyUnit     PrtMarkerSuppliesSupplyUnitTC,
    prtMarkerSuppliesMaxCapacity    Integer32,
    prtMarkerSuppliesLevel          Integer32
    }

prtMarkerSuppliesIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this marker
        supply.  Although these values may change due to a major
        reconfiguration of the device (e.g., the addition of new marker

        supplies to the printer), values SHOULD remain stable across
        successive printer power cycles.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMarkerSuppliesEntry 1 }

prtMarkerSuppliesMarkerIndex OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The value of prtMarkerIndex corresponding to the marking sub
        unit with which this marker supply sub-unit is associated."
    ::= { prtMarkerSuppliesEntry 2 }

prtMarkerSuppliesColorantIndex OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The value of prtMarkerColorantIndex corresponding to the
        colorant with which this marker supply sub-unit is associated.
        This value shall be 0 if there is no colorant table or if this
        supply does not depend on a single specified colorant.
        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMarkerSuppliesEntry 3 }

prtMarkerSuppliesClass OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtMarkerSuppliesClassTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Indicates whether this supply entity represents a supply that
        is consumed or a receptacle that is filled.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMarkerSuppliesEntry 4 }

prtMarkerSuppliesType OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtMarkerSuppliesTypeTC
    MAX-ACCESS read-only

    STATUS     current
    DESCRIPTION
        "The type of this supply."
    ::= { prtMarkerSuppliesEntry 5 }

prtMarkerSuppliesDescription OBJECT-TYPE
    -- In RFC 1759, the SYNTAX was OCTET STRING.  This has been changed
    -- to a TC to better support localization of the object.
    SYNTAX     PrtLocalizedDescriptionStringTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The description of this supply container/receptacle in the
        localization specified by prtGeneralCurrentLocalization."
    ::= { prtMarkerSuppliesEntry 6 }

prtMarkerSuppliesSupplyUnit OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtMarkerSuppliesSupplyUnitTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Unit of measure of this marker supply container/receptacle.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMarkerSuppliesEntry 7 }

prtMarkerSuppliesMaxCapacity OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The maximum capacity of this supply container/receptacle
        expressed in prtMarkerSuppliesSupplyUnit.  If this supply
        container/receptacle can reliably sense this value, the value
        is reported by the printer and is read-only; otherwise, the
        value may be written (by a Remote Control Panel or a Management
        Application).  The value (-1) means other and specifically
        indicates that the sub-unit places no restrictions on this
        parameter.  The value (-2) means unknown."
    ::= { prtMarkerSuppliesEntry 8 }

prtMarkerSuppliesLevel OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-3..2147483647)

    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The current level if this supply is a container; the remaining
        space if this supply is a receptacle.  If this supply
        container/receptacle can reliably sense this value, the value
        is reported by the printer and is read-only; otherwise, the
        value may be written (by a Remote Control Panel or a Management
        Application).  The value (-1) means other and specifically
        indicates that the sub-unit places no restrictions on this
        parameter.  The value (-2) means unknown.  A value of (-3) means
        that the printer knows that there is some supply/remaining
        space, respectively."
    ::= { prtMarkerSuppliesEntry 9 }

-- The Marker Colorant Group

prtMarkerColorant OBJECT IDENTIFIER ::= { printmib 12 }

prtMarkerColorantTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtMarkerColorantEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of all of the colorants available on the printer."
    ::= { prtMarkerColorant 1 }

prtMarkerColorantEntry OBJECT-TYPE
    SYNTAX     PrtMarkerColorantEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Attributes of a colorant available on the printer.  Entries may
        exist in the table for each device index with a device type of
        'printer'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX { hrDeviceIndex, prtMarkerColorantIndex }
    ::= { prtMarkerColorantTable 1 }

PrtMarkerColorantEntry ::= SEQUENCE {
    prtMarkerColorantIndex          Integer32,
    prtMarkerColorantMarkerIndex    Integer32,
    prtMarkerColorantRole           PrtMarkerColorantRoleTC,
    prtMarkerColorantValue          OCTET STRING,
    prtMarkerColorantTonality       Integer32
    }

prtMarkerColorantIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this colorant.
        Although these values may change due to a major reconfiguration
        of the device (e.g., the addition of new colorants to the
        printer) , values SHOULD remain stable across successive
        printer power cycles.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMarkerColorantEntry 1 }

prtMarkerColorantMarkerIndex OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The value of prtMarkerIndex corresponding to the marker sub
        unit with which this colorant entry is associated."
    ::= { prtMarkerColorantEntry 2 }

prtMarkerColorantRole OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtMarkerColorantRoleTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The role played by this colorant."
    ::= { prtMarkerColorantEntry 3 }

prtMarkerColorantValue OBJECT-TYPE
    -- NOTE: The string length range has been increased from RFC 1759.
    SYNTAX     OCTET STRING (SIZE(0..255))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The name of the color of this colorant using standardized
        string names from ISO 10175 (DPA) and ISO 10180 (SPDL) such as:
            other
            unknown
            white
            red
            green
            blue

            cyan
            magenta
            yellow
            black
        Implementers may add additional string values.  The naming
        conventions in ISO 9070 are recommended in order to avoid
        potential name clashes"
    ::= { prtMarkerColorantEntry 4 }

prtMarkerColorantTonality OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The distinct levels of tonality realizable by a marking sub
        unit when using this colorant.  This value does not include the
        number of levels of tonal difference that an interpreter can
        obtain by techniques such as half toning.  This value must be at
        least 2."
    ::= { prtMarkerColorantEntry 5 }

-- The Media Path Group
--
-- The media paths encompass the mechanisms in the printer that
-- move the media through the printer and connect all other media
-- related sub-units: inputs, outputs, markers and finishers.  A
-- printer contains one or more media paths.  These are
-- represented by the Media Path Group in the model.

prtMediaPath OBJECT IDENTIFIER ::= { printmib 13 }

prtMediaPathTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtMediaPathEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The media path table includes both physical and logical paths
        within the printer.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMediaPath 4 }

prtMediaPathEntry OBJECT-TYPE
    SYNTAX     PrtMediaPathEntry
    MAX-ACCESS not-accessible
    STATUS     current

    DESCRIPTION
        "Entries may exist in the table for each device index with a
        device type of 'printer'  Each entry defines the physical
        characteristics of and the status of the media path.  The data
        provided indicates the maximum throughput and the media
        size limitations of these subunits.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX  { hrDeviceIndex, prtMediaPathIndex }
    ::= { prtMediaPathTable 1 }

PrtMediaPathEntry ::= SEQUENCE {
    prtMediaPathIndex               Integer32,
    prtMediaPathMaxSpeedPrintUnit   PrtMediaPathMaxSpeedPrintUnitTC,
    prtMediaPathMediaSizeUnit       PrtMediaUnitTC,
    prtMediaPathMaxSpeed            Integer32,
    prtMediaPathMaxMediaFeedDir     Integer32,
    prtMediaPathMaxMediaXFeedDir    Integer32,
    prtMediaPathMinMediaFeedDir     Integer32,
    prtMediaPathMinMediaXFeedDir    Integer32,
    prtMediaPathType                PrtMediaPathTypeTC,
    prtMediaPathDescription         PrtLocalizedDescriptionStringTC,
    prtMediaPathStatus              PrtSubUnitStatusTC
    }

prtMediaPathIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this media
        path.  Although these values may change due to a major
        reconfiguration of the device (e.g., the addition of new media
        paths to the printer), values SHOULD remain stable across
        successive printer power cycles.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMediaPathEntry 1 }

prtMediaPathMaxSpeedPrintUnit OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX PrtMediaPathMaxSpeedPrintUnitTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION

        "The unit of measure used in specifying the speed of all media
        paths in the printer."
    ::= { prtMediaPathEntry 2 }

prtMediaPathMediaSizeUnit OBJECT-TYPE
    SYNTAX     PrtMediaUnitTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The units of measure of media size for use in calculating and
        relaying dimensional values for all media paths in the
        printer."
    ::= { prtMediaPathEntry 3 }

prtMediaPathMaxSpeed OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The maximum printing speed of this media path expressed in
        prtMediaPathMaxSpeedUnit's.  A value of (-1) implies 'other'."
    ::= { prtMediaPathEntry 4 }

prtMediaPathMaxMediaFeedDir OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The maximum physical media size in the feed direction of this
        media path expressed in units of measure specified by
        PrtMediaPathMediaSizeUnit.  A value of (-1) implies 'unlimited'
        a value of (-2) implies 'unknown'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMediaPathEntry 5 }

prtMediaPathMaxMediaXFeedDir OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The maximum physical media size across the feed direction of
        this media path expressed in units of measure specified by
        prtMediaPathMediaSizeUnit.  A value of (-2) implies 'unknown'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMediaPathEntry 6 }

prtMediaPathMinMediaFeedDir OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The minimum physical media size in the feed direction of this
        media path expressed in units of measure specified by
        prtMediaPathMediaSizeUnit.  A value of (-2) implies 'unknown'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMediaPathEntry 7 }

prtMediaPathMinMediaXFeedDir OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The minimum physical media size across the feed direction of
        this media path expressed in units of measure specified by
        prtMediaPathMediaSizeUnit.  A value of (-2) implies 'unknown'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtMediaPathEntry 8 }

prtMediaPathType OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtMediaPathTypeTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The type of the media path for this media path."
    ::= { prtMediaPathEntry 9 }

prtMediaPathDescription OBJECT-TYPE
    -- In RFC 1759, the SYNTAX was OCTET STRING.  This has been changed
    -- to a TC to better support localization of the object.
    SYNTAX     PrtLocalizedDescriptionStringTC
    MAX-ACCESS read-only
    STATUS     current

    DESCRIPTION
        "The manufacturer-provided description of this media path in
        the localization specified by prtGeneralCurrentLocalization."
    ::= { prtMediaPathEntry 10 }

prtMediaPathStatus OBJECT-TYPE
    SYNTAX     PrtSubUnitStatusTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "The current status of this media path."
    ::= { prtMediaPathEntry 11 }

-- The Print Job Delivery Channel Group
--
-- Print Job Delivery Channels are independent sources of print
-- data.  Here, print data is the term used for the information
-- that is used to construct printed pages and may have both data
-- and control aspects.  The output of a channel is in a form
-- suitable for input to one of the interpreters as a
-- stream.  A channel may be independently enabled (allowing
-- print data to flow) or disabled (stopping the flow of
-- print data).  A printer may have one or more channels.
--
-- The Print Job Delivery Channel table describes the
-- capabilities of the printer and not what is currently being
-- performed by the printer
--
-- Basically, the print job delivery channel abstraction
-- describes the final processing step of getting the print data
-- to an interpreter.  It might include some level of
-- decompression or decoding of print stream data.
-- channel.  All of these aspects are hidden in the channel
-- abstraction.
--
-- There are many kinds of print job delivery channels; some of
-- which are based on networks and others which are not.  For
-- example, a channel can be a serial (or parallel) connection;
-- it can be a service, such as the UNIX Line Printer Daemon
-- (LPD), offering services over a network connection; or
-- it could be a disk drive into which a floppy disk with
-- the print data is inserted.  Each print job delivery channel is
-- identified by the electronic path and/or service protocol
-- used to deliver print data to a print data interpreter.
--
-- Channel example                   Implementation
--
-- serial port channel            bi-directional data channel

-- parallel port channel          often uni-directional channel
-- IEEE 1284 port channel         bi-directional channel
-- SCSI port channel              bi-directional
-- Apple PAP channel              may be based on LocalTalk,
--                                Ethernet or Tokentalk
-- LPD Server channel             TCP/IP based, port 515
-- Netware Remote Printer         SPX/IPX based channel
-- Netware Print Server           SPX/IPX based channel
--
-- It is easy to note that this is a mixed bag.  There are
-- some physical connections over which no (or very meager)
-- protocols are run (e.g., the serial or old parallel ports)
-- and there are services which often have elaborate
-- protocols that run over a number of protocol stacks.  In
-- the end, what is important is the delivery of print data
-- through the channel.
--
-- The print job delivery channel sub-units are represented by
-- the Print Job Delivery Channel Group in the Model.  It has a
-- current print job control language, which can be used to
-- specify which interpreter is to be used for the print data and
-- to query and change environment variables used by the
-- interpreters (and Management Applications).  There is also a
-- default interpreter that is to be used if an interpreter is
-- not explicitly specified using the Control Language.

-- The first seven items in the Print Job Delivery Channel Table
-- define the "channel" itself.  A channel typically depends on
-- other protocols and interfaces to provide the data that flows
-- through the channel.
--
-- Control of a print job delivery channel is largely limited to
-- enabling or disabling the entire channel itself.  It is likely
-- that more control of the process of accessing print data
-- will be needed over time.  Thus, the ChannelType will
-- allow type-specific data to be associated with each
-- channel (using ChannelType specific groups in a fashion
-- analogous to the media specific MIBs that are associated
-- with the IANAIfType in the Interfaces Table).  As a first
-- step in this direction, each channel will identify the
-- underlying Interface on which it is based.  This is the
-- eighth object in each row of the table.

-- The Print Job Delivery Channel Table

prtChannel OBJECT IDENTIFIER ::= { printmib 14 }

prtChannelTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtChannelEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The channel table represents the set of input data sources
        which can provide print data to one or more of the
        interpreters available on a printer.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtChannel 1 }

prtChannelEntry OBJECT-TYPE
    SYNTAX     PrtChannelEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Entries may exist in the table for each device index with a
        device type of 'printer'.  Each channel table entry is
        characterized by a unique protocol stack and/or addressing.
        The channel may also have printer dependent features that are
        associated with a printing language.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX  { hrDeviceIndex, prtChannelIndex }
    ::= { prtChannelTable 1 }

PrtChannelEntry ::= SEQUENCE {
    prtChannelIndex                     Integer32,
    prtChannelType                      PrtChannelTypeTC,
    prtChannelProtocolVersion           OCTET STRING,
    prtChannelCurrentJobCntlLangIndex   Integer32,
    prtChannelDefaultPageDescLangIndex  Integer32,
    prtChannelState                     PrtChannelStateTC,
    prtChannelIfIndex                   InterfaceIndexOrZero,
    prtChannelStatus                    PrtSubUnitStatusTC,
    prtChannelInformation               OCTET STRING
    }

prtChannelIndex OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (1..65535)

    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this data
        channel.  Although these values may change due to a major
        reconfiguration of the device (e.g., the addition of new data
        channels to the printer), values SHOULD remain stable across
        successive printer power cycles.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtChannelEntry 1 }

prtChannelType OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtChannelTypeTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The type of this print data channel.  This object provides the
        linkage to ChannelType-specific groups that may (conceptually)
        extend the prtChannelTable with additional details about that
        channel."
    ::= { prtChannelEntry 2 }

prtChannelProtocolVersion OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The version of the protocol used on this channel.  The format
        used for version numbering depends on prtChannelType."
    ::= { prtChannelEntry 3 }

prtChannelCurrentJobCntlLangIndex OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of prtInterpreterIndex corresponding to the Control
        Language Interpreter for this channel.  This interpreter defines
        the syntax used for control functions, such as querying or
        changing environment variables and identifying job boundaries
        (e.g., PJL, PostScript, NPAP).  A value of zero indicates that
        there is no current Job Control Language Interpreter for this
        channel.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtChannelEntry 4 }

prtChannelDefaultPageDescLangIndex OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of prtInterpreterIndex corresponding to the Page
        Description Language Interpreter for this channel.  This
        interpreter defines the default Page Description Language
        interpreter to be used for the print data unless the Control
        Language is used to select a specific interpreter (e.g., PCL,
        PostScript Language, auto-sense).  A value of zero indicates
        that there is no default page description language interpreter
        for this channel.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtChannelEntry 5 }

prtChannelState OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtChannelStateTC
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The state of this print data channel.  The value determines
        whether control information and print data is allowed through
        this channel or not."
    ::= { prtChannelEntry 6 }

prtChannelIfIndex OBJECT-TYPE
    SYNTAX     InterfaceIndexOrZero   -- Was Integer32 in RFC 1759.
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of ifIndex in the ifTable; see the Interfaces Group
        MIB [RFC2863] which corresponds to this channel.
        When more than one row of the ifTable is relevant, this is the
        index of the row representing the topmost layer in the
        interface hierarchy.  A value of zero indicates that no
        interface is associated with this channel.

        NOTE: The above description has been modified from RFC 1759

        for clarification."
    ::= { prtChannelEntry 7 }

prtChannelStatus OBJECT-TYPE
    SYNTAX     PrtSubUnitStatusTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The current status of the channel."
    ::= { prtChannelEntry 8 }

prtChannelInformation OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..255))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Auxiliary information to allow a printing application to use
        the channel for data submission to the printer.  An application
        capable of using a specific PrtChannelType should be able to
        use the combined information from the prtChannelInformation and
        other channel and interface group objects to 'bootstrap' its
        use of the channel.  prtChannelInformation is not intended to
        provide a general channel description, nor to provide
        information that is available once the channel is in use.

        The encoding and interpretation of the prtChannelInformation
        object is specific to channel type.  The description of each
        PrtChannelType enum value for which prtChannelInformation is
        defined specifies the appropriate encoding and interpretation,
        including interaction with other objects.  For channel types
        that do not specify a prtChannelInformation value, its value
        shall be null (0 length).

        When a new PrtChannelType enumeration value is registered, its
        accompanying description must specify the encoding and
        interpretation of the prtChannelInformation value for the
        channel type.  prtChannelInformation semantics for an existing
        PrtChannelType may be added or amended in the same manner as
        described in section 2.4.1 for type 2 enumeration values.

        The prtChannelInformation specifies values for a collection of
        channel attributes, represented as text according to the
        following rules:

        1. The prtChannelInformation is not affected by localization.

        2. The prtChannelInformation is a list of entries representing
        the attribute values.  Each entry consists of the following

        items, in order:

        a. A keyword, composed of alphabetic characters (A-Z, a-z)
        represented by their NVT ASCII [RFC854] codes, that
        identifies a channel attribute,

        b. The NVT ASCII code for an Equals Sign (=) (code 61) to
        delimit the keyword,

        c. A data value encoded using rules specific to the
        PrtChannelType to with the prtChannelInformation applies which
        must in no case allow an octet with value 10 (the NVT ASCII
        Line Feed code),

        d. the NVT ASCII code for a Line Feed character (code 10) to
        delimit the data value.

        No other octets shall be present.

        Keywords are case-sensitive.  Conventionally, keywords are
        capitalized (including each word of a multi-word keyword) and
        since they occupy space in the prtChannelInformation, they are
        kept short.

        3. If a channel attribute has multiple values, it is
        represented by multiple entries with the same keyword, each
        specifying one value. Otherwise, there shall be at most one
        entry for each attribute.

        4. By default, entries may appear in any order.  If there are
        ordering constraints for particular entries, these must be
        specified in their definitions.

        5. The prtChannelInformation value by default consists of text
        represented by NVT ASCII graphics character codes.  However,
        other representations may be specified:

        a. In cases where the prtChannelInformation value contains
        information not normally coded in textual form, whatever
        symbolic representation is conventionally used for the
        information should be used for encoding the
        prtChannelInformation value.  (For instance, a binary port value
        might be represented as a decimal number using NVT ASCII
        codes.)  Such encoding must be specified in the definition of
        the value.

        b. The value may contain textual information in a character set
        other than NVT ASCII graphics characters.  (For instance, an

        identifier might consist of ISO 10646 text encoded using the
        UTF-8 encoding scheme.)  Such a character set and its encoding
        must be specified in the definition of the value.

        6. For each PrtChannelType for which prtChannelInformation
        entries are defined, the descriptive text associated with the
        PrtChannelType enumeration value shall specify the following
        information for each entry:

        Title:        Brief description phrase, e.g.: 'Port name',
                      'Service Name', etc.

        Keyword:      The keyword value, e.g.: 'Port' or 'Service'

        Syntax:       The encoding of the entry value if it cannot be
                      directly represented by NVT ASCII.

        Status:       'Mandatory', 'Optional', or 'Conditionally
                      Mandatory'

        Multiplicity: 'Single' or 'Multiple' to indicate whether the
                      entry may be present multiple times.

        Description:  Description of the use of the entry, other
                      information required to complete the definition
                      (e.g.: ordering constraints, interactions between
                      entries).

        Applications that interpret prtChannelInformation should ignore
        unrecognized entries, so they are not affected if new entry
        types are added."

     ::= { prtChannelEntry 9 }

-- The Interpreter Group
--
-- The interpreter sub-units are responsible for the conversion
-- of a description of intended print instances into images that
-- are to be marked on the media.  A printer may have one or more
-- interpreters.  The interpreter sub-units are represented by the
-- Interpreter Group in the Model.  Each interpreter is generally
-- implemented with software running on the System Controller
-- sub-unit.  The Interpreter Table has one entry per interpreter
-- where the interpreters include both Page Description Language
-- (PDL) Interpreters and Control Language Interpreters.

prtInterpreter OBJECT IDENTIFIER ::= { printmib 15 }

--       Interpreter Table

prtInterpreterTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtInterpreterEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The interpreter table is a table representing the
        interpreters in the printer.  An entry shall be placed in the
        interpreter table for each interpreter on the printer.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtInterpreter 1 }

prtInterpreterEntry OBJECT-TYPE
    SYNTAX     PrtInterpreterEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Entries may exist in the table for each device index with a
        device type of 'printer'.  Each table entry provides a complete
        description of the interpreter, including version information,
        rendering resolutions, default character sets, output
        orientation, and communication capabilities.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX  { hrDeviceIndex, prtInterpreterIndex }
    ::= { prtInterpreterTable 1 }

PrtInterpreterEntry ::= SEQUENCE {
    prtInterpreterIndex                 Integer32,
    prtInterpreterLangFamily            PrtInterpreterLangFamilyTC,
    prtInterpreterLangLevel             OCTET STRING,
    prtInterpreterLangVersion           OCTET STRING,
    prtInterpreterDescription           PrtLocalizedDescriptionStringTC,
    prtInterpreterVersion               OCTET STRING,
    prtInterpreterDefaultOrientation    PrtPrintOrientationTC,
    prtInterpreterFeedAddressability    Integer32,
    prtInterpreterXFeedAddressability   Integer32,
    prtInterpreterDefaultCharSetIn      IANACharset,
    prtInterpreterDefaultCharSetOut     IANACharset,
    prtInterpreterTwoWay                PrtInterpreterTwoWayTC
    }

prtInterpreterIndex OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.

    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value for each PDL or control language for which
        there exists an interpreter or emulator in the printer.  The
        value is used to identify this interpreter.  Although these
        values may change due to a major reconfiguration of the device
        (e.g., the addition of new interpreters to the printer), values
        SHOULD remain stable across successive printer power cycles.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtInterpreterEntry 1 }

prtInterpreterLangFamily OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtInterpreterLangFamilyTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The family name of a Page Description Language (PDL) or
        control language which this interpreter in the printer can
        interpret or emulate.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtInterpreterEntry 2 }

prtInterpreterLangLevel OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..31))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The level of the language which this interpreter is
        interpreting or emulating.  This might contain a value like
        '5e'for an interpreter which is emulating level 5e of the PCL
        language.  It might contain '2' for an interpreter which is
        emulating level 2 of the PostScript language.  Similarly it
        might contain '2' for an interpreter which is emulating level 2
        of the HPGL language."
    ::= { prtInterpreterEntry 3 }

prtInterpreterLangVersion OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..31))
    MAX-ACCESS read-only
    STATUS     current

    DESCRIPTION
        "The date code or version of the language which this
        interpreter is interpreting or emulating."
    ::= { prtInterpreterEntry 4 }

prtInterpreterDescription OBJECT-TYPE
    -- In RFC 1759, the SYNTAX was OCTET STRING.  This has been changed
    -- to a TC to better support localization of the object.
    SYNTAX     PrtLocalizedDescriptionStringTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A string to identify this interpreter in the localization
        specified by prtGeneralCurrentLocalization as opposed to the
        language which is being interpreted.  It is anticipated that
        this string will allow manufacturers to unambiguously identify
        their interpreters."
    ::= { prtInterpreterEntry 5 }

prtInterpreterVersion OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..31))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The date code, version number, or other product specific
        information tied to this interpreter.  This value is associated
        with the interpreter, rather than with the version of the
        language which is being interpreted or emulated."
    ::= { prtInterpreterEntry 6 }

prtInterpreterDefaultOrientation OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtPrintOrientationTC
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The current orientation default for this interpreter.  This
        value may be overridden for a particular job (e.g., by a
        command in the input data stream)."
    ::= { prtInterpreterEntry 7 }

prtInterpreterFeedAddressability OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION

        "The maximum interpreter addressability in the feed
        direction in 10000 prtMarkerAddressabilityUnits (as specified
        by prtMarkerDefaultIndex) for this interpreter.  The
        value (-1) means other and specifically indicates that the
        sub-unit places no restrictions on this parameter.  The value
        (-2) means unknown.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtInterpreterEntry 8 }

prtInterpreterXFeedAddressability OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The maximum interpreter addressability in the cross feed
        direction in 10000 prtMarkerAddressabilityUnits (as specified
        by prtMarkerDefaultIndex) for this interpreter.  The
        value (-1) means other and specifically indicates that the
        sub-unit places no restrictions on this parameter.  The value
        (-2) means unknown.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtInterpreterEntry 9 }

prtInterpreterDefaultCharSetIn OBJECT-TYPE
    SYNTAX     IANACharset
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The default coded character set for input octets encountered
        outside a context in which the Page Description Language
        established the interpretation of the octets.  (Input octets are
        presented to the interpreter through a path defined in the
        channel group.)"
     ::= { prtInterpreterEntry 10 }

prtInterpreterDefaultCharSetOut OBJECT-TYPE
    SYNTAX     IANACharset
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The default character set for data coming from this
        interpreter through the printer's output channel (i.e. the
        'backchannel')."

    ::= { prtInterpreterEntry 11 }

prtInterpreterTwoWay OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtInterpreterTwoWayTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Indicates whether or not this interpreter returns information
        back to the host."
    ::= { prtInterpreterEntry 12 }

-- The Console Group
--
-- Many printers have a console on the printer, the operator
-- console, that is used to display and modify the state of the
-- printer.  The console can be as simple as a few indicators and
-- switches or as complicated as full screen displays and
-- keyboards.  There can be at most one such console.

-- The Display Buffer Table

prtConsoleDisplayBuffer OBJECT IDENTIFIER ::= { printmib 16 }

prtConsoleDisplayBufferTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtConsoleDisplayBufferEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Physical display buffer for printer console display or
        operator panel

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtConsoleDisplayBuffer 5 }

prtConsoleDisplayBufferEntry OBJECT-TYPE
    SYNTAX     PrtConsoleDisplayBufferEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This table contains one entry for each physical line on
        the display.  Lines cannot be added or deleted.  Entries may
        exist in the table for each device index with a device type of
        'printer'.

        NOTE: The above description has been modified from RFC 1759

        for clarification."
    INDEX  { hrDeviceIndex, prtConsoleDisplayBufferIndex }
    ::= { prtConsoleDisplayBufferTable 1 }

PrtConsoleDisplayBufferEntry ::= SEQUENCE {
    prtConsoleDisplayBufferIndex    Integer32,
    prtConsoleDisplayBufferText     PrtConsoleDescriptionStringTC
    }

prtConsoleDisplayBufferIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value for each console line in the printer.  The value
        is used to identify this console line.  Although these values
        may change due to a major reconfiguration of the device (e.g.,
        the addition of new console lines to the printer).  Values
        SHOULD remain stable across successive printer power cycles.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtConsoleDisplayBufferEntry 1 }

prtConsoleDisplayBufferText OBJECT-TYPE
    -- In RFC 1759, the SYNTAX was OCTET STRING.  This has been changed
    -- to a TC to better support localization of the object.
    SYNTAX     PrtConsoleDescriptionStringTC
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The content of a line in the logical display buffer of
        the operator's console of the printer.  When a write
        operation occurs, normally a critical message, to one of
        the LineText strings, the agent should make that line
        displayable if a physical display is present.  Writing a zero
        length string clears the line.  It is an implementation-
        specific matter as to whether the agent allows a line to be
        overwritten before it has been cleared.  Printer generated
        strings shall be in the localization specified by
        prtConsoleLocalization.Management Application generated strings
        should be localized by the Management Application."
    ::= { prtConsoleDisplayBufferEntry 2 }

-- The Console Light Table

prtConsoleLights OBJECT IDENTIFIER ::= { printmib 17 }

prtConsoleLightTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtConsoleLightEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The console light table provides a description and state
        information for each light present on the printer console.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtConsoleLights 6 }

prtConsoleLightEntry OBJECT-TYPE
    SYNTAX     PrtConsoleLightEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Entries may exist in the table for each device index with a
        device type of 'printer'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX  { hrDeviceIndex, prtConsoleLightIndex }
    ::= { prtConsoleLightTable 1 }

PrtConsoleLightEntry ::= SEQUENCE {
    prtConsoleLightIndex            Integer32,
    prtConsoleOnTime                Integer32,
    prtConsoleOffTime               Integer32,
    prtConsoleColor                 PrtConsoleColorTC,
    prtConsoleDescription           PrtConsoleDescriptionStringTC
    }

prtConsoleLightIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)  -- Lower limit invalid in RFC 1759
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this light.
        Although these values may change due to a major
        reconfiguration of the device (e.g., the addition of new lights
        to the printer).  Values SHOULD remain stable across successive
        printer power cycles.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtConsoleLightEntry 1 }

prtConsoleOnTime OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (0..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This object, in conjunction with prtConsoleOffTime, defines
        the current status of the light.  If both prtConsoleOnTime and
        prtConsoleOffTime are non-zero, the lamp is blinking and the
        values presented define the on time and off time, respectively,
        in milliseconds.  If prtConsoleOnTime is zero and
        prtConsoleOffTime is non-zero, the lamp is off.  If
        prtConsoleOffTime is zero and prtConsoleOnTime is non-zero, the
        lamp is on.  If both values are zero the lamp is off.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtConsoleLightEntry 2 }

prtConsoleOffTime OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (0..2147483647)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This object, in conjunction with prtConsoleOnTime, defines the
        current status of the light.  If both prtConsoleOnTime and
        prtConsoleOffTime are non-zero, the lamp is blinking and the
        values presented define the on time and off time, respectively,
        in milliseconds.  If prtConsoleOnTime is zero and
        prtConsoleOffTime is non-zero, the lamp is off.  If
        prtConsoleOffTime is zero and prtConsoleOnTime is non-zero, the
        lamp is on.  If both values are zero the lamp is off.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtConsoleLightEntry 3 }

prtConsoleColor OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtConsoleColorTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The color of this light."
    ::= { prtConsoleLightEntry 4 }

prtConsoleDescription OBJECT-TYPE
    -- In RFC 1759, the SYNTAX was OCTET STRING.  This has been changed
    -- to a TC to better support localization of the object.
    SYNTAX     PrtConsoleDescriptionStringTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The vendor description or label of this light in the
        localization specified by prtConsoleLocalization."
    ::= { prtConsoleLightEntry 5 }

-- The Alerts Group
--
-- The table contains information on the severity, component,
-- detail location within the component, alert code and
-- description of each critical alert that is currently active
-- within the printer.  See 2.2.13 for a more complete
-- description of the alerts table and its management.
--
-- Each parameter in the Trap PDU is a full OID which itself is
-- indexed by the host resources MIB "hrDeviceIndex" object.  In
-- order for a management station to obtain the correct
-- "hrDeviceIndex" associated with a particular Trap PDU, the
-- "hrDeviceIndex" value can be extracted from the returned OID
-- value in the Trap PDU when the PDU is received by the
-- Management station.

prtAlert OBJECT IDENTIFIER ::= { printmib 18 }

prtAlertTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtAlertEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The prtAlertTable lists all the critical and non-critical
        alerts currently active in the printer.  A critical alert is
        one that stops the printer from printing immediately and
        printing can not continue until the critical alert condition
        is eliminated.  Non-critical alerts are those items that do
        not stop printing but may at some future time.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtAlert 1 }

prtAlertEntry OBJECT-TYPE
    SYNTAX     PrtAlertEntry
    MAX-ACCESS not-accessible

    STATUS     current
    DESCRIPTION
        "Entries may exist in the table for each device
        index with a device type of 'printer'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    INDEX  { hrDeviceIndex, prtAlertIndex }
    ::= { prtAlertTable 1 }

PrtAlertEntry ::= SEQUENCE {
    prtAlertIndex               Integer32,
    prtAlertSeverityLevel       PrtAlertSeverityLevelTC,
    prtAlertTrainingLevel       PrtAlertTrainingLevelTC,
    prtAlertGroup               PrtAlertGroupTC,
    prtAlertGroupIndex          Integer32,
    prtAlertLocation            Integer32,
    prtAlertCode                PrtAlertCodeTC,
    prtAlertDescription         PrtLocalizedDescriptionStringTC,
    prtAlertTime                TimeTicks
    }

prtAlertIndex OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.  The MAX-ACCESS has
    --       been changed from not accessible to allow the object to be
    --       included (as originally in RFC 1759) in the trap bindings.

    SYNTAX     Integer32 (1..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The index value used to determine which alerts have been added
        or removed from the alert table.  This is an incrementing
        integer initialized to 1 when the printer is reset.  (i.e., The
        first event placed in the alert table after a reset of the
        printer shall have an index value of 1.)  When the printer adds
        an alert to the table, that alert is assigned the next higher
        integer value from the last item entered into the table.  If
        the index value reaches its maximum value, the next index value
        used must be 1.

        NOTE: The management application will read the alert table when
        a trap or event notification occurs or at a periodic rate and
        then parse the table to determine if any new entries were added
        by comparing the last known index value with the current
        highest index value.  The management application will then
        update its copy of the alert table.  When the printer discovers
        that an alert is no longer active, the printer shall remove the

        row for that alert from the table and shall reduce the number
        of rows in the table.  The printer may add or delete any number
        of rows from the table at any time.  The management station can
        detect when binary change alerts have been deleted by
        requesting an attribute of each alert, and noting alerts as
        deleted when that retrieval is not possible.  The objects
        'prtAlertCriticalEvents'and 'prtAlertAllEvents' in the
        'prtGeneralTable' reduce the need for management applications
        to scan the 'prtAlertTable'.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtAlertEntry 1 }

prtAlertSeverityLevel OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtAlertSeverityLevelTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The level of severity of this alert table entry.  The printer
        determines the severity level assigned to each entry into the
        table."
    ::= { prtAlertEntry 2 }

prtAlertTrainingLevel OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtAlertTrainingLevelTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "See TEXTUAL-CONVENTION PrtAlertTrainingLevelTC.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtAlertEntry 3 }

prtAlertGroup OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtAlertGroupTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The type of sub-unit within the printer model that this alert
        is related.  Input, output, and markers are examples of printer

        model groups, i.e., examples of types of sub-units.  Wherever
        possible, these enumerations match the sub-identifier that
        identifies the relevant table in the printmib."
    ::= { prtAlertEntry 4 }

prtAlertGroupIndex OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-1..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The low-order index of the row within the table identified
        by prtAlertGroup that represents the sub-unit of the printer
        that caused this alert, or -1 if not applicable.  The
        combination of the prtAlertGroup and the prtAlertGroupIndex
        defines exactly which printer sub-unit caused the alert; for
        example, Input #3, Output#2, and Marker #1.  Every object in
        this MIB is indexed with hrDeviceIndex and optionally, another
        index variable.  If this other index variable is present in the
        table that generated the alert, it will be used as the value
        for this object.  Otherwise, this value shall be -1.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtAlertEntry 5 }

prtAlertLocation OBJECT-TYPE
    -- NOTE: In RFC 1759, the range was not defined.
    SYNTAX     Integer32 (-2..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The sub-unit location that is defined by the printer
        manufacturer to further refine the location of this alert
        within the designated sub-unit.  The location is used in
        conjunction with the Group and GroupIndex values; for example,
        there is an alert in Input #2 at location number 7.  The value
        (-2) indicates unknown.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtAlertEntry 6 }

prtAlertCode OBJECT-TYPE
    --  NOTE: In RFC 1759, the enumeration values were implicitly
    --  defined by this object.
    SYNTAX     PrtAlertCodeTC
    MAX-ACCESS read-only

    STATUS     current
    DESCRIPTION
        "See associated TEXTUAL-CONVENTION PrtAlertCodeTC.

        NOTE: The above description has been modified from RFC 1759
        for clarification."
    ::= { prtAlertEntry 7 }

prtAlertDescription OBJECT-TYPE
    -- In RFC 1759, the SYNTAX was OCTET STRING.  This has been changed
    -- to a TC to better support localization of the object.
    SYNTAX     PrtLocalizedDescriptionStringTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A description of this alert entry in the localization
        specified by prtGeneralCurrentLocalization.  The description is
        provided by the printer to further elaborate on the enumerated
        alert or provide information in the case where the code is
        classified as 'other' or 'unknown'.  The printer is required to
        return a description string but the string may be a null
        string."
    ::= { prtAlertEntry 8 }

prtAlertTime OBJECT-TYPE
    SYNTAX     TimeTicks
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The value of sysUpTime at the time that this alert was
        generated."
    ::= { prtAlertEntry 9 }

printerV1Alert OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The value of the enterprise-specific OID in an SNMPv1 trap
        sent signaling a critical event in the prtAlertTable."
    ::= { prtAlert 2 }

printerV2AlertPrefix OBJECT IDENTIFIER ::= { printerV1Alert 0 }

printerV2Alert NOTIFICATION-TYPE
    OBJECTS { prtAlertIndex, prtAlertSeverityLevel, prtAlertGroup,
        prtAlertGroupIndex, prtAlertLocation, prtAlertCode }
    STATUS  current
    DESCRIPTION
        "This trap is sent whenever a critical event is added to the

        prtAlertTable.

        NOTE: The prtAlertIndex object was redundantly included in the
        bindings of the 'printerV2Alert' notification in RFC 1759, even
        though the value exists in the instance qualifier of all the
        other bindings.  This object has been retained to provide
        compatiblity with existing RFC 1759 implementaions."
    ::= { printerV2AlertPrefix 1 }

-- Note that the SNMPv2 to SNMPv1 translation rules dictate that
-- the preceding structure will result in SNMPv1 traps of the
-- following form:
--
-- printerAlert TRAP-TYPE
--     ENTERPRISE printerV1Alert
--     VARIABLES { prtAlertIndex, prtAlertSeverityLevel,
--                 prtAlertGroup, prtAlertGroupIndex,
--                 prtAlertLocation, prtAlertCode }
--     DESCRIPTION
--        "This trap is sent whenever a critical event is added
--         to the prtAlertTable."
--     ::= 1

-- Conformance Information

prtMIBConformance OBJECT IDENTIFIER ::= { printmib 2 }

-- compliance statements

prtMIBCompliance MODULE-COMPLIANCE

    STATUS  current
    DESCRIPTION
        "The compliance statement for agents that implement the
        printer MIB as defined by RFC 1759."
    MODULE -- this module
    MANDATORY-GROUPS { prtGeneralGroup, prtInputGroup,
                       prtOutputGroup,
                       prtMarkerGroup, prtMediaPathGroup,
                       prtChannelGroup, prtInterpreterGroup,
                       prtConsoleGroup, prtAlertTableGroup }
    OBJECT    prtGeneralReset
    SYNTAX    INTEGER {
                  notResetting(3),
                  resetToNVRAM(5)
                  }
    DESCRIPTION
        "It is conformant to implement just these two states in this

        object.  Any additional states are optional."

    OBJECT    prtConsoleOnTime
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtConsoleOffTime
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"
    ::= { prtMIBConformance 1 }

prtMIB2Compliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
        "The compliance statement for agents that implement the
        printer MIB V2."
        -- The changes from RFC 1759 fall into 2 categories:
        -- 1. New objects plus existing objects with a MIN-ACCESS of
        --    read-only are included.  Existing objects have been added
        --    to this category due to feedback from implementers and
        --    interoperability testing.  This allows products to be
        --    be designed with a higher degree of SNMP security.
        -- 2. New object groups have been added to include all new
        --    objects in this MIB.  All new object groups are optional.
        -- Any MIB that is compliant with RFC 1759 will also be
        -- compliant with this version of the MIB.
    MODULE -- this module
    MANDATORY-GROUPS { prtGeneralGroup, prtInputGroup,
                       prtOutputGroup,
                       prtMarkerGroup, prtMediaPathGroup,
                       prtChannelGroup, prtInterpreterGroup,
                       prtConsoleGroup, prtAlertTableGroup }
    OBJECT    prtGeneralReset
    SYNTAX    INTEGER {
                  notResetting(3),
                  resetToNVRAM(5)
                  }
    DESCRIPTION
        "It is conformant to implement just these two states in this
        object.  Any additional states are optional."

    OBJECT    prtGeneralCurrentLocalization
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtGeneralCurrentOperator
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtGeneralServicePerson
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtGeneralPrinterName
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtGeneralSerialNumber
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInputDefaultIndex
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInputMediaDimFeedDirDeclared
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInputMaxCapacity
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInputCurrentLevel
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInputMediaName
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInputName
    MIN-ACCESS  read-only
    DESCRIPTION

        "It is conformant to implement this object as read-only"

    OBJECT    prtInputSecurity
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInputMediaWeight
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInputMediaType
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInputMediaColor
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInputMediaFormParts
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputDefaultIndex
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputMaxCapacity
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputRemainingCapacity
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputName
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputSecurity

    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputMaxDimFeedDir
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputMaxDimXFeedDir
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputMinDimFeedDir
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputMinDimXFeedDir
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputStackingOrder
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputPageDeliveryOrientation
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputBursting
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputDecollating
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputPageCollated
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtOutputOffsetStacking
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtMarkerDefaultIndex
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtMarkerSuppliesMaxCapacity
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtMarkerSuppliesLevel
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtMediaPathDefaultIndex
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtChannelCurrentJobCntlLangIndex
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtChannelDefaultPageDescLangIndex
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtChannelState
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtChannelIfIndex
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInterpreterDefaultOrientation
    MIN-ACCESS  read-only
    DESCRIPTION

        "It is conformant to implement this object as read-only"

    OBJECT    prtInterpreterDefaultCharSetIn
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInterpreterDefaultCharSetOut
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtConsoleLocalization
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtConsoleDisable
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtConsoleDisplayBufferText
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtConsoleOnTime
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtConsoleOffTime
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtAlertIndex
    MIN-ACCESS  accessible-for-notify
    DESCRIPTION
        "It is conformant to implement this object as
        accessible-for-notify "

    GROUP    prtResponsiblePartyGroup
    DESCRIPTION
        "This group is unconditionally optional."

    GROUP    prtExtendedInputGroup

    DESCRIPTION
        "This group is unconditionally optional."

    GROUP    prtInputMediaGroup
    DESCRIPTION
        "This group is unconditionally optional."

    GROUP    prtExtendedOutputGroup
    DESCRIPTION
        "This group is unconditionally optional."

    GROUP    prtOutputDimensionsGroup
    DESCRIPTION
        "This group is unconditionally optional."

    GROUP    prtOutputFeaturesGroup
    DESCRIPTION
        "This group is unconditionally optional."

    GROUP    prtMarkerSuppliesGroup
    DESCRIPTION
        "This group is unconditionally optional."

    GROUP    prtMarkerColorantGroup
    DESCRIPTION
        "This group is unconditionally optional."

    GROUP    prtAlertTimeGroup
    DESCRIPTION
        "This group is unconditionally optional."

    -- the prtResponsiblePartyGroup, prtExtendedInputGroup,
    -- prtInputMediaGroup, prtExtendedOutputGroup,
    -- prtOutputDimensionsGroup, prtOutputFeaturesGroup,
    -- prtMarkerSuppliesGroup, prtMarkerColorantGroup, and the
    -- prtAlertTimeGroup are completely optional.  However, it is
    -- strongly RECOMMENDED that the prtAlertTimeGroup be implemented.

    -- New to version 2 of this printer MIB:
    OBJECT    prtAuxiliarySheetStartupPage
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtAuxiliarySheetBannerPage
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInputMediaLoadTimeout
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    OBJECT    prtInputNextIndex
    MIN-ACCESS  read-only
    DESCRIPTION
        "It is conformant to implement this object as read-only"

    GROUP    prtAuxiliarySheetGroup
    DESCRIPTION
        "This group is unconditionally optional."

    GROUP    prtInputSwitchingGroup
    DESCRIPTION
        "This group is unconditionally optional."

    GROUP    prtGeneralV2Group
    DESCRIPTION
        "This group is unconditionally optional."

    GROUP    prtAlertTableV2Group
    DESCRIPTION
        "This group is unconditionally optional."

    GROUP    prtChannelV2Group
    DESCRIPTION
        "This group is unconditionally optional."

    GROUP    prtAlertTrapGroup
    DESCRIPTION
        "This group is unconditionally optional."
    ::= { prtMIBConformance 3 }

prtMIBGroups    OBJECT IDENTIFIER ::= { prtMIBConformance 2 }
-- These groups are from RFC 1759 and are applicable to Printer MIB V2

prtGeneralGroup OBJECT-GROUP
    OBJECTS { prtGeneralConfigChanges,
              prtGeneralCurrentLocalization,
              prtGeneralReset, prtCoverDescription,
              prtCoverStatus,
              prtLocalizationLanguage, prtLocalizationCountry,
              prtLocalizationCharacterSet, prtStorageRefIndex,
              prtDeviceRefIndex }
    STATUS  current
    DESCRIPTION

        "The general printer group."
    ::= { prtMIBGroups 1 }

prtResponsiblePartyGroup OBJECT-GROUP
    OBJECTS { prtGeneralCurrentOperator, prtGeneralServicePerson }
    STATUS  current
    DESCRIPTION
        "The responsible party group contains contact information for
        humans responsible for the printer."
    ::= { prtMIBGroups 2 }

prtInputGroup OBJECT-GROUP
    OBJECTS { prtInputDefaultIndex, prtInputType, prtInputDimUnit,
              prtInputMediaDimFeedDirDeclared,
              prtInputMediaDimXFeedDirDeclared,
              prtInputMediaDimFeedDirChosen,
              prtInputMediaDimXFeedDirChosen, prtInputCapacityUnit,
              prtInputMaxCapacity, prtInputCurrentLevel, prtInputStatus,
              prtInputMediaName }
    STATUS  current
    DESCRIPTION
        "The input group."
    ::= { prtMIBGroups 3 }

prtExtendedInputGroup OBJECT-GROUP
    OBJECTS { prtInputName, prtInputVendorName, prtInputModel,
              prtInputVersion, prtInputSerialNumber,
              prtInputDescription, prtInputSecurity }
    STATUS  current
    DESCRIPTION
        "The extended input group."
    ::= { prtMIBGroups 4 }

prtInputMediaGroup OBJECT-GROUP
    OBJECTS { prtInputMediaWeight, prtInputMediaType,
              prtInputMediaColor, prtInputMediaFormParts }
    STATUS  current
    DESCRIPTION
        "The input media group."
    ::= { prtMIBGroups 5 }

prtOutputGroup OBJECT-GROUP
    OBJECTS { prtOutputDefaultIndex, prtOutputType,
              prtOutputCapacityUnit, prtOutputMaxCapacity,
              prtOutputRemainingCapacity,  prtOutputStatus }
    STATUS  current
    DESCRIPTION
        "The output group."

    ::= { prtMIBGroups 6 }

prtExtendedOutputGroup OBJECT-GROUP
    OBJECTS { prtOutputName, prtOutputVendorName, prtOutputModel,
              prtOutputVersion, prtOutputSerialNumber,
              prtOutputDescription, prtOutputSecurity }
    STATUS  current
    DESCRIPTION
        "The extended output group."
    ::= { prtMIBGroups 7 }

prtOutputDimensionsGroup OBJECT-GROUP
    OBJECTS { prtOutputDimUnit, prtOutputMaxDimFeedDir,
              prtOutputMaxDimXFeedDir, prtOutputMinDimFeedDir,
              prtOutputMinDimXFeedDir }
    STATUS  current
    DESCRIPTION
        "The output dimensions group"
    ::= { prtMIBGroups 8 }

prtOutputFeaturesGroup OBJECT-GROUP
    OBJECTS { prtOutputStackingOrder,
              prtOutputPageDeliveryOrientation, prtOutputBursting,
              prtOutputDecollating, prtOutputPageCollated,
              prtOutputOffsetStacking }
    STATUS  current
    DESCRIPTION
        "The output features group."
    ::= { prtMIBGroups 9 }

prtMarkerGroup OBJECT-GROUP
    OBJECTS { prtMarkerDefaultIndex, prtMarkerMarkTech,
              prtMarkerCounterUnit, prtMarkerLifeCount,
              prtMarkerPowerOnCount, prtMarkerProcessColorants,
              prtMarkerSpotColorants, prtMarkerAddressabilityUnit,
              prtMarkerAddressabilityFeedDir,
              prtMarkerAddressabilityXFeedDir, prtMarkerNorthMargin,
              prtMarkerSouthMargin, prtMarkerWestMargin,
              prtMarkerEastMargin, prtMarkerStatus }
    STATUS  current
    DESCRIPTION
        "The marker group."
    ::= { prtMIBGroups 10 }

prtMarkerSuppliesGroup OBJECT-GROUP
    OBJECTS { prtMarkerSuppliesMarkerIndex,
              prtMarkerSuppliesColorantIndex, prtMarkerSuppliesClass,
              prtMarkerSuppliesType, prtMarkerSuppliesDescription,

              prtMarkerSuppliesSupplyUnit,
              prtMarkerSuppliesMaxCapacity, prtMarkerSuppliesLevel }
    STATUS  current
    DESCRIPTION
        "The marker supplies group."
    ::= { prtMIBGroups 11 }

prtMarkerColorantGroup OBJECT-GROUP
    OBJECTS { prtMarkerColorantMarkerIndex, prtMarkerColorantRole,
              prtMarkerColorantValue, prtMarkerColorantTonality }
    STATUS  current
    DESCRIPTION
        "The marker colorant group."
    ::= { prtMIBGroups 12 }

prtMediaPathGroup OBJECT-GROUP
    OBJECTS { prtMediaPathDefaultIndex, prtMediaPathMaxSpeedPrintUnit,
              prtMediaPathMediaSizeUnit, prtMediaPathMaxSpeed,
              prtMediaPathMaxMediaFeedDir,
              prtMediaPathMaxMediaXFeedDir,
              prtMediaPathMinMediaFeedDir,
              prtMediaPathMinMediaXFeedDir, prtMediaPathType,
              prtMediaPathDescription, prtMediaPathStatus}
    STATUS  current
    DESCRIPTION
        "The media path group."
    ::= { prtMIBGroups 13 }

prtChannelGroup OBJECT-GROUP
    OBJECTS { prtChannelType, prtChannelProtocolVersion,
              prtChannelCurrentJobCntlLangIndex,
              prtChannelDefaultPageDescLangIndex, prtChannelState,
              prtChannelIfIndex, prtChannelStatus
              }
    STATUS  current
    DESCRIPTION
        "The channel group."
    ::= { prtMIBGroups 14 }

prtInterpreterGroup OBJECT-GROUP
    OBJECTS { prtInterpreterLangFamily, prtInterpreterLangLevel,
              prtInterpreterLangVersion, prtInterpreterDescription,
              prtInterpreterVersion, prtInterpreterDefaultOrientation,
              prtInterpreterFeedAddressability,
              prtInterpreterXFeedAddressability,
              prtInterpreterDefaultCharSetIn,
              prtInterpreterDefaultCharSetOut, prtInterpreterTwoWay }
    STATUS  current

    DESCRIPTION
        "The interpreter group."
    ::= { prtMIBGroups 15 }

prtConsoleGroup OBJECT-GROUP
    OBJECTS { prtConsoleLocalization, prtConsoleNumberOfDisplayLines,
              prtConsoleNumberOfDisplayChars, prtConsoleDisable,
              prtConsoleDisplayBufferText, prtConsoleOnTime,
              prtConsoleOffTime, prtConsoleColor,
              prtConsoleDescription }
    STATUS  current
    DESCRIPTION
        "The console group."
    ::= { prtMIBGroups 16 }

prtAlertTableGroup OBJECT-GROUP
    OBJECTS { prtAlertSeverityLevel, prtAlertTrainingLevel,
              prtAlertGroup, prtAlertGroupIndex, prtAlertLocation,
              prtAlertCode, prtAlertDescription }
    STATUS  current
    DESCRIPTION
        "The alert table group."
    ::= { prtMIBGroups 17 }

prtAlertTimeGroup OBJECT-GROUP
    OBJECTS { prtAlertTime }
    STATUS  current
    DESCRIPTION
        "The alert time group. Implementation of prtAlertTime is
        strongly RECOMMENDED."
    ::= { prtMIBGroups 18 }

prtMIB2Groups    OBJECT IDENTIFIER ::= { prtMIBConformance 4 }
-- These groups are unique to Printer MIB V2

prtAuxiliarySheetGroup OBJECT-GROUP
    OBJECTS { prtAuxiliarySheetStartupPage,
              prtAuxiliarySheetBannerPage }
    STATUS  current
    DESCRIPTION
        "The auxiliary sheet group."
    ::= { prtMIBGroups 19 }

prtInputSwitchingGroup OBJECT-GROUP
    OBJECTS { prtInputMediaLoadTimeout, prtInputNextIndex }
    STATUS  current
    DESCRIPTION
        "The input switching group."

    ::= { prtMIBGroups 20 }

prtGeneralV2Group OBJECT-GROUP
    OBJECTS { prtGeneralPrinterName, prtGeneralSerialNumber }
    STATUS  current
    DESCRIPTION
        "The general printer group with new v2 objects."
    ::= { prtMIBGroups 21 }

prtAlertTableV2Group OBJECT-GROUP
    OBJECTS { prtAlertIndex, prtAlertCriticalEvents, prtAlertAllEvents }
    STATUS  current
    DESCRIPTION
        "The alert table group with new v2 objects and prtAlertIndex
        changed to MAX-ACCESS of 'read-only' for inclusion in the trap
        bindings (as originally defined in RFC 1759)."

    ::= { prtMIBGroups 22 }

prtChannelV2Group OBJECT-GROUP
    OBJECTS { prtChannelInformation }
    STATUS  current
    DESCRIPTION
        "The channel group with a new v2 object."
    ::= { prtMIBGroups 23 }

prtAlertTrapGroup NOTIFICATION-GROUP
    NOTIFICATIONS { printerV2Alert }
    STATUS  current
    DESCRIPTION
        "The alert trap group."
    ::= { prtMIBGroups 24 }

END


