eG Monitoring

Measures reported by GtmDtCntrStatTest A data center is a facility that provides shared access to applications and data using a complex network, compute, and storage infrastructure. This test auto-discovers the data centers in the target BIG-IP GTM and for each data center, this test reports the availability and the status of the data center. Using this test, administrators can instantly identify the data centers that are not available/error-prone/disabled. Outputs of the test: One set of results for each data center in BIG-IP GTM that is being monitored. Descriptor: Data Center The measures made by this test are as follows:
Measurement | Description | Measurement Unit | Interpretation
--- | --- | --- | ---
Datacenter_avail | Indicates the availability of this data center. |  | The values reported by this measure and its numeric equivalent are mentioned in the table below:
Measure Value | Numeric Value
Available | 0
Unknown | 1
Unlicensed | 2
Error | 3
Currently not available | 4
Not available | 5
Note: By default, this measure reports the above-mentioned Measure Values while indicating the availability of this data center in BIG-IP GTM. However, in the graph of this measure, measure values will be represented using the corresponding numeric equivalents only - i.e., 0 to 5.
Datacenter_state | Indicates the activity status of this data center. |  | The values reported by this measure and its numeric equivalent are mentioned in the table below:
Measure Value | Numeric Value
None | 0
Enabled | 1
Disabled | 2
Disabled by parent | 3
Note: By default, this measure reports the above-mentioned Measure Values while indicating the activity status of this data center in BIG-IP GTM. However, in the graph of this measure, measure values will be represented using the corresponding numeric equivalents only - i.e., 0 to 3.