eG Monitoring

Measures reported by OraZFSNICStTest This test monitors the network interfaces supported by the Oracle ZFS Storage system and reports the rate at which network packets and data were transmitted/received over every discovered interface, and the errors encountered by each. This way, the test sheds light on the slow, error-prone, and congested (in terms of level of network traffic) network interfaces of the Oracle ZFS Storage system. Outputs of the test: One set of results for the Oracle ZFS Storage System being monitored. The measures made by this test are as follows:
Measurement | Description | Measurement Unit | Interpretation
--- | --- | --- | ---
nicData | Indicates the average data transfer rate. | MB/sec |
utilByNICDeviceMax | Indicates the maximum bandwidth utilization by device during the last measurement period. | MB/Sec | Compare the value of this measure across the network to know which device is consuming the maximum bandwidth. The detailed diagnosis shows the names of devices consuming maximum bandwidth.
utilByNICDirectionMax | Indicates the maximum bandwidth utilization by direction during the last measurement period. | MB/Sec | Compare the value of this measure across the network to know when the devices are consuming maximum bandwidth. The detailed diagnosis shows if the devices are consuming maximum bandwidth during input/ output operations.