Agents Administration - Tests

Configuration of AzrADInfoTest Use this test to audit the inventory managed by Azure AD, and to track the usage of AD objects. The test proactively alerts you to abnormal object usage. The test also reveals whether the on-premises environment has successfully synched its identity data with Azure AD. If so, then the detailed diagnostics of the test will reveal when last was identity data synched between your on-premises environment and Azure AD. These details will help you figure out if there are any irregularities in synchronization services. The default parameters associated with this test are: The TEST PERIOD list box helps the user to decide how often this test needs to be executed. In the HOST text box, specify the HOST for which this test is to be configured. Specify the Directory ID of the Azure AD tenant to which the target subscription belongs in the TENANT ID text box. To know how to determine the Directory ID/Tenant ID Click here. The eG agent communicates with the target Microsoft Azure Subscrption using Java API calls. To collect the required metrics, the eG agent requires an Access token in the form of an Application ID and the client secret value.Specify the Application ID of the created Application in the CLIENT ID TEXTBOX To know how to determine the Application ID Click here. Specify the client secret value in the CLIENT PASSWORD text box. To obtain the client secret value Click here. In some environments, all communication with the Azure cloud be routed through a proxy server. In such environments, you should make sure that the eG agent connects to the cloud via the proxy server and collects metrics. To enable metrics collection via a proxy, specify the IP address of the proxy server and the port at which the server listens against the PROXY HOST and PROXY PORT parameters. By default, these parameters are set to none , indicating that the eG agent is not configured to communicate via a proxy, by default. If the proxy server requires authentication, then, specify a valid proxy user name and password in the PROXY USERNAME and PROXY PASSWORD parameters, respectively. Then, confirm the password by retyping it in the Confirm Password text box. Refers to the frequency with which detailed diagnosis measures are to be generated for this test. The default is 6:1. This indicates that, by default, detailed measures will be generated every sixth time this test runs, and also every time the test detects a problem. You can modify this frequency, if you so desire. Also, if you intend to disable the detailed diagnosis capability for this test, you can do so by specifying none against DD FREQUENCY. To make diagnosis more efficient and accurate, the eG Enterprise embeds an optional detailed diagnostic capability. With this capability, the eG agents can be configured to run detailed, more elaborate tests as and when specific problems are detected. To enable the detailed diagnosis capability of this test for a particular server, choose the On option. To disable the capability, click on the Off option. The option to selectively enable/disable the detailed diagnosis capability will be available only if the following conditions are fulfilled: The eG manager license should allow the detailed diagnosis capability Both the normal and abnormal frequencies configured for the detailed diagnosis measures should not be 0. If multiple components of the same component type are awaiting configuration, then an APPLY TO OTHER COMPONENTS button will appear in this page. Clicking on this button will allow you to apply the configuration to all/selected components of that type. Once the necessary values have been provided, clicking on the UPDATE button will register the changes made. When changing the configuration for specific servers, a “*” beside the text box corresponding to the parameter signifies that these values have to be manually configured by the user. The parameter values that require to be configured will typically be prefixed with a “$” or contain a series of “*”. A value of “none” in the parameter value indicates that the corresponding parameter value can be changed if required.