eG Monitoring

Measures reported by ScpVmStTest Using the Virtual Machine Status test, the administrator can identify any reboots that occurred in the virtual machine and track if the virtual machine has stopped or encountered operation failures. Outputs of the test :One set of results for each Virtual Machine in the target SAP BTP Neo Environment. The measures made by this test are as follows:
Measurement | Description | Measurement Unit | Interpretation
--- | --- | --- | ---
state | Indicates the status of virtual machine. |  | The values reported by this measure and its numeric equivalents are mentioned in the table below:
Measure Value | Numeric Value
Starting | 0
Started | 1
Rebooting | 2
Deleting | 3
Stopped | 4
Failed | 5
Note: By default, this measure reports the Measure Values listed in the table above to indicate whether/not the virtual machine had started. The detailed diagnosis of this measure provides the virtual machine status details like the security vm group id, security vm size(GB), ip address, image id, public key, created date, last modified, access point id and access point url.