eG Monitoring

Measures reported by BB12XMDSPushConTest The BlackBerry MDS Connection Service sends data to each BlackBerry device specified in the push request as a series of packets.To control the flow of pushed data, the BlackBerry MDS Connection Service initially sends a maximum of five packets. By default, a BlackBerry MDS (Mobile Data System) Connection Service sends push requests from server-side push applications to applications on BlackBerry devices. BlackBerry devices can receive application data and application updates without users requesting the content. This test monitors the MDS push connections and reports the number and size of the data packets and the number of push connections that were created and cached. This test helps to find out if there is any loss in data packets. Outputs of the test: One set of results for Blackberry UEM 12.x device. The measures made by this test are as follows:
Measurement | Description | Measurement Unit | Interpretation
--- | --- | --- | ---
packetsSizetoDvcsOnPush | Indicates the total size of the data packets sent to BlackBerry devices during the last measurement period. | MB | This measure denotes the size of the packets sent to the Blackberry devices. These packets are sent to all Blackberry devices through push connections initiated by the BlackBerry MDS Connection Service, in KB and it is converted to MB.
packetstoDeviceOnPush | This measure denotes the total number of data packets sent to BlackBerry devices during the last measurement period. | Number |
pushConnectionsbyMDS | Indicates the total number of push connections initiated by the BlackBerry MDS Connection Service during the last measurement period. | Number |
cachedPushConnection | Indicates the number of push connections that were created and cached. | Number |