eG Monitoring

Measures reported by OraZFSHardStTest This test monitors the overall status of the hardware and serves as an effective health indicator for the following system components: Disk Fan Memory PSU This test alerts the administrator in case of faults in any of the hardware components. Outputs of the test: One set of results for each controller: hardware type: hardware component in the Oracle ZFS Storage System being monitored. Descriptors: controller: hardware type: hardware component The measures made by this test are as follows:
Measurement | Description | Measurement Unit | Interpretation
--- | --- | --- | ---
isPresent | Indicates the status of the device present in the controller. |  | The values reported by this measure and its numeric equivalent are mentioned in the table below:
Measure Value | Numeric Value
No | 0
Yes | 100
Note: By default, this measure reports the above-mentioned States while indicating whether the Oracle ZFS storage component is available or not. However, in the graph of this measure, states will be represented using the corresponding numeric equivalents only i.e., 0 or 1.
isFaulted | Indicates whether the device is faulty or not. |  | The values reported by this measure and its numeric equivalent are mentioned in the table below:
Measure Value | Numeric Value
No | 0
Yes | 100
Note: By default, this measure reports the above-mentioned States while indicating whether the status of the Oracle ZFS storage component is in faulty condition. However, in the graph of this measure, states will be represented using the corresponding numeric equivalents only i.e., 0 or 100.