Agents Administration - Tests

Configuration of OraZFSFCStatTest This test monitors and reports the data transfer rate and the I/O transfer rate through Fiber channel between the Storage and LUN. Using this test, the administrator would be able to track the bandwidth usage between the storage and LUN. The default parameters associated with this test are: The TEST PERIOD list box helps the user to decide how often this test needs to be executed. In the HOST text box, specify the IP address of the host for which this test is to be configured. In the PORT text box, specify the port at which the specified host is listening. By default, this is set to 215. By default, this test uses the REST API commands to pull out the required metrics. To execute the REST API commands, the eG agent requires the permission of a local administrator user who has been assigned with Basic role and a custom role with Analytics authorization and read permission. Specify the credentials of such a user in the USERNAME and PASSWORD text boxes and confirm the Password by retyping it in the CONFIRM PASSWORD text box. To create a new user with the required permissions, click here. Specify the time duration for which this test should wait for a response from the storage system in the TIMEOUT text box. By default, this is 60 seconds. If multiple components of the same component type are awaiting configuration, then an APPLY TO OTHER COMPONENTS button will appear in this page. Clicking on this button will allow you to apply the configuration to all/selected components of that type. Once the necessary values have been provided, clicking on the UPDATE button will register the changes made. When changing the configuration for specific servers, a “*” beside the text box corresponding to the parameter signifies that these values have to be manually configured by the user. The parameter values that require to be configured will typically be prefixed with a “$” or contain a series of “*”. A value of “none” in the parameter value indicates that the corresponding parameter value can be changed if required.