eG Monitoring

Measures reported by GtmDnsQryRespnsTest Using this test, administrators can monitor the DNS query responses that are sent by the target BIG-IP GTM. Using this test, administrators can figure out how many signatures have been succeeded/failed. Outputs of the test: One set of results for the BIG-IP GTM that is being monitored. The measures made by this test are as follows:
Measurement | Description | Measurement Unit | Interpretation
--- | --- | --- | ---
Total_sign_crypto_failed | Indicates the number of signatures that failed due to cryptographic operation failure during the last measurement period. | Number | Ideally, the value of this measure is desired to be zero.
Total_sign_success | Indicates the number of successfully generated signatures during the last measurement period. | Number | A high value is desired for this measure.
Total_sign_failed | Indicates the number of signatures that had failed during the last measurement period. | Number | Ideally, the value of this measure is desired to be zero.
Total_sign_rrset_failed | Indicates the number of failures due to an RRSET failing to be signed during the last measurement period. | Number | An RRSET (Resource Record Set) is a set of resource records in a DNS zone that have the same name and type. Ideally, a value close to zero is desired.