eG Monitoring

Measures reported by OraZFSiSCSITest The iSCSI (Internet Small Computer Systems Interface) protocol is a licensed service on the storage system that enables you to transfer block data to hosts using the SCSI protocol over TCP/IP. This test monitors the active and attempted iSCSI sessions, and promptly captures the bandwidth used and the Input/ Output operations encountered by these sessions. Outputs of the test: One set of results for the Oracle ZFS Storage System being monitored. The measures made by this test are as follows:
Measurement | Description | Measurement Unit | Interpretation
--- | --- | --- | ---
iSCSIData | Indicates the data transferred between the Storage and LUN via iSCSI (Internet Small Computer Systems Interface) per second. | MB/sec | A higher value denotes excessive bandwidth utilization.
iSCSIIOPS | Indicates the input and output rate through iSCSI between the Storage and LUN. | IOPS | A sudden high value could indicate a processing bottleneck. The gradual increase in the value of this measure indicates a consistent rise of I/O load.