eG Monitoring

Measures reported by OraZFSAltLogTest This test monitors and reports the alert logs that helps the administrator to troubleshoot the device for any major alerts, if noticed. Using this test, the administrator can find out how many major/ minor alerts have been raised, why and when it had been raised along with its severity. Outputs of the test: One set of results for the Oracle ZFS Storage System being monitored. The measures made by this test are as follows:
Measurement | Description | Measurement Unit | Interpretation
--- | --- | --- | ---
majorAlerts | Indicates how many major alerts had been found during the last measurement period. | Number | Ideally the value of this measure should be 0. An abnormally high value could indicate that the component is problem prone. Use the detailed diagnosis of this measure to know the why the alert has been raised, UUID of the alert, type, and severity of the alert along with the time the alert had been raised.
minorAlerts | Indicates how many minor alerts had been found during the last measurement period. | Number | Ideally the value of this measure should be 0. Use the detailed diagnosis of this measure to know the why the alert has been raised, UUID of the alert, type and severity of the alert along with the time the alert had been raised.
otherAlerts | Indicates how many other alerts had been found during the last measurement period. | Number | Ideally the value of this measure should be 0. Use the detailed diagnosis of this measure to know the why the alert has been raised, UUID of the alert, type and severity of the alert along with the time the alert had been raised.