eG Administration

Discovering EMC XtremIO hosts using XMS Management Servers eG Enterprise is capable of automatically discovering the EMC XtremIO Clusters available in the target environment using the XMS Management Server. The eG Enterprise system can auto-discover the EMC XtremIO clusters managed in the XMS Management Server using the IP address of the XMS Management Server. To enable this auto-discovery, you first need to enable the eG manager to connect to a XMS Management Server in the target environment, The Storage Discovery sub-node in the DISCOVERY tree can be used for this purpose. Follow the steps mentioned below to discover the EMC XtremIO clusters using the XMS Management Server: Once you clicked the Storage Discovery sub-node, the EMC XtremIO 4x option will be chosen by default from the Choose a storage platform to discover list. Then, select the Add new XMS option from the What action would you like to perform? drop down list. To configure a new XMS Management Server, specify the following in the XMS Preferences section: Specify the IP or host name of the XMS Management Server in the XMS Identity (IP or Host name) text box. Then, indicate whether the eG manager is to connect to the XMS Management Server using SSL or not by selecting the Yes or No option from the Use SSL to connect to XMS list. By default, this list is set to Yes. An IT environment may consist of multiple XMS Management Servers, each managing a different set of EMC XtremIO Clusters. To enable the eG manager to automatically discover those EMC XtremIO Clusters that are managed using the XMS Management Server being added, set the Discover EMC XtremIO hosts using this XMS flag to Yes. If not, then set this flag to No. In order to be able to discover the EMC XtremIO hosts using the XMS Management Server, the eG manager needs to connect to the XMS Management Server using the credentials of a valid user to the XMS Management Server. Provide the user name and password of such a user in the Username to connect to XMS and Password for the user text boxes. Confirm the password of the user by retyping it in the Confirm password for the user text box. To clear all the configuration details, click on the Clear button. To start discovery instead, click on the Update button. Clicking on the Update button requests you to confirm whether you want to start discovery based on the specifications provided. Click the Yes button to begin discovery. Regardless of the discovery approach used (discovery using an IP range or using XMS Management Server), triggering EMC XtremIO storage systems discovery will lead you straight to the COMPONENTS - MANAGE / UNMANAGE page. To view the XMS Management Server so added, select the View configured XMS from the What action would you like to perform? list. Then the list of XMS servers that have been configured for discovering EMC XtremIO hosts will appear. To modify a XMS Management Server configuration, select the Modify configured XMS option from the What action would you like to perform? drop down list. Then, select the IP/host name of the XMS Management Server to be modified from the XMS identity (IP or Host name) list. The details of the chosen XMS Management Server will then be displayed against the appropriate fields. You can modify any of the displayed details and update the changes by clicking the Update button. To delete a particular XMS Management Server, select the Delete configured XMS option from the What action would you like to perform? dropdown. Then, the list of available XMS Management Servers will appear. Select the XMS Management Server to be deleted by selecting the check boxes corresponding to the XMS Management Server configuration. To mark all the listed XMS Management Servers for deletion simultaneously, simply select the top-most check box in the column of check boxes. To delete the marked XMS Management Servers, click on the Delete button.